Notes For V3.5-1

The source set has been extensively overhauled.  For correct
viewing, set Visual C++ or Emacs to have tab stops every 4
characters.

1. New Features

1.1 3.5-0

1.1.1 All Ethernet devices

- Added Windows user-defined adapter names (from Timothe Litt)

1.1.2 Interdata, SDS, HP, PDP-8, PDP-18b terminal multiplexors

- Added support for SET <unit>n DISCONNECT

1.1.3 VAX

- Added latent QDSS support
- Revised autoconfigure to handle QDSS

1.1.4 PDP-11

- Revised autoconfigure to handle more casees

2. Bugs Fixed

2.1 3.5-0

2.1.1 SCP and libraries

- Trim trailing spaces on all input (for example, attach file names)
- Fixed sim_sock spurious SIGPIPE error in Unix/Linux
- Fixed sim_tape misallocation of TPC map array for 64b simulators

2.1.2 1401

- Fixed bug, CPU reset was clearing SSB through SSG

2.1.3 PDP-11

- Fixed bug in VH vector display routine
- Fixed XU runt packet processing (found by Tim Chapman)

2.1.4 Interdata

- Fixed bug in SHOW PAS CONN/STATS
- Fixed potential integer overflow exception in divide

2.1.5 SDS

- Fixed bug in SHOW MUX CONN/STATS

2.1.6 HP

- Fixed bug in SHOW MUX CONN/STATS

2.1.7 PDP-8

- Fixed bug in SHOW TTIX CONN/STATS
- Fixed bug in SET/SHOW TTOXn LOG

2.1.8 PDP-18b

- Fixed bug in SHOW TTIX CONN/STATS
- Fixed bug in SET/SHOW TTOXn LOG

2.1.9 Nova, Eclipse

- Fixed potential integer overflow exception in divide

2.2 3.5-1

2.2.1 1401

- Changed character encodings to be compatible with Pierce 709X simulator
- Added mode for old/new character encodings

2.2.2 1620

- Changed character encodings to be compatible with Pierce 709X simulator

2.2.3 PDP-10

- Changed MOVNI to eliminate GCC warning

2.2.4 VAX

- Fixed bug in structure definitions with 32b compilation options
- Fixed bug in autoconfiguration table

2.2.5 PDP-11

- Fixed bug in autoconfiguration table



