D e l i v e r i n g M e d i a G e n e r i c a l l y o v e r R T P d r a f t - p e r i y a n n a n - g e n e r i c - r t p - 0 0 41st IETF, Los AngelesApril 1998A l a g u P e r i y a n n a n David SingerApple Computer, Inc.Michael SpeerSun Microsystems, Inc.

A. Periyannan41st IETF, Los Angeles, April 1998M o t i v a t i o n a n d G o a l s ¥ An interoperable scheme for sending new codecsand media types over RTP¥ Based on discussion at the 40th IETF inWashington, D.C. (December 1997)¥ Goals- Define a set of RTP packetization schemes- Define a mechanism within SDP to conveyencoding information to receivers

A. Periyannan41st IETF, Los Angeles, April 1998G e n e r i c S c h e m e A ¥ Recommended Usage- Duration & Size of each sample is constant- Size of each sample < MTU size¥ Example: Frame or sample-based Audio

A. Periyannan41st IETF, Los Angeles, April 1998G e n e r i c S c h e m e A P a c k e t F o r m a t 0 1 2 30 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. RTP Header .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. Sample Data... .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+¥ One or more samples follow RTP header¥ M-bit unused

A. Periyannan41st IETF, Los Angeles, April 1998Generic Scheme B¥ Recommended Usage- Size of samples is variable (typically > MTU)- Duration is the timestamp difference orcontained in the sample- No external key sample detection¥ Example: Frame-based video with large frames i z e s

A. Periyannan41st IETF, Los Angeles, April 1998

A. Periyannan41st IETF, Los Angeles, April 1998Generic Scheme BP a c k e t F o r m a t 0 1 2 30 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. RTP Header .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. Sample Data... .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+¥ One complete sample or sample fragment followsRTP header¥ M-bit set on last packet of sample

A. Periyannan41st IETF, Los Angeles, April 1998G e n e r i c S c h e m e C ¥ Recommended Usage- Size of samples is variable (Some samples >MTU, many samples << MTU)- Duration needs to be specified explicitly- External key sample detection required

A. Periyannan41st IETF, Los Angeles, April 1998G e n e r i c S c h e m e C ( c o n t d . ) ¥ Examples:- Frame-based video with some large frames andmany small frames- Proprietary video streams that require a keys a m p l e m a r k i n g m e c h a n i s m - MIDI streams that require duration to bespecified for a sample

A. Periyannan41st IETF, Los Angeles, April 1998G e n e r i c S c h e m e C P a c k e t F o r m a t 0 1 2 30 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. RTP Header .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. Scheme C Header... .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. Sample Data... .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. Scheme C Header... .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. Sample Data... .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+. ...... .+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+

A. Periyannan41st IETF, Los Angeles, April 1998G e n e r i c S c h e m e C P a c k e t F o r m a t ( c o n t d . ) ¥ Scheme C header precedes each sample or samplef r a g m e n t ¥ RTP data contains- One complete sample or sample fragment ineach RTP packeto r - Multiple samples in each RTP packet¥ M-bit set on last packet of sample

A. Periyannan41st IETF, Los Angeles, April 1998S c h e m e C H e a d e r 0 1 2 30 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1 2 3 4 5 6 7 8 9 0 1+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+|S|L|R|D| RES | Length/Offset |+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+| Relative Timestamp |+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+| Duration |+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+¥ S-bit indicates key sample¥ L-bit set for Length, set to zero for Offset¥ R-bit indicates presence of Relative Timestamp¥ D-bit indicates presence of Duration

A. Periyannan41st IETF, Los Angeles, April 1998S D P M o d i f i c a t i o n s ¥ SDP used to convey the following:- RTP Packetization Scheme- Media sample encoding format- Parameters for the media encoding format

A. Periyannan41st IETF, Los Angeles, April 1998r t p m a p & f m t p ¥ Current usage of rtpmap:a=rtpmap:<payload type> <encoding name>/<clockrate>[/<encoding parameters>]¥ New usage for <encoding name>:"[<namespace>/]<encoding format>[,<packetizations c h e m e > ] " ¥ <format specific parameters> in fmtp is scoped by<encoding format>a=fmtp:<format> <format specific parameters>

A. Periyannan41st IETF, Los Angeles, April 1998

A. Periyannan41st IETF, Los Angeles, April 1998r t p m a p e x a m p l e s a=rtpmap:99 "indeo,genpak-b"/600a=rtpmap:99 "x-qt/midi,genpak-c"/30a=rtpmap:99 "x-asf/00000002-0000-0010-8000-0 0 A A 0 0 3 8 9 B 7 1 , g e n p a k - a " / 8 0 0 0 a=rtpmap:99 "x-qt/viderpza,genpak-b"/90000a=rtpmap:99 "x-qt/twen,x-qtsprite"/600

A. Periyannan41st IETF, Los Angeles, April 1998O p e n I s s u e s ¥ M-bit usage in scheme A¥ A new rtpmap2¥ Multiple fmtp attribute lines per format¥ Binary data in fmtp attribute lines¥ Large SDP files