/*
 * $Id: input.txt 9312 2008-09-05 00:08:34Z vszakats $
 */

/*
 * The following parts are Copyright of the individual authors.
 * www - http://www.harbour-project.org
 *
 * Copyright 1999 Chen Kedem <niki@actcom.co.il>
 *    Documentation for: READKEY()
 *
 * See doc/license.txt for licensing terms.
 *
 */

/*  $DOC$
 *  $FUNCNAME$
 *      INKEY()
 *  $CATEGORY$
 *      Console input
 *  $ONELINER$
 *      Extracts the next key code from the Harbour keyboard buffer.
 *  $SYNTAX$
 *      INKEY( [<nTimeout>] [,<nEvents>] ) --> nKey
 *  $ARGUMENTS$
 *      <nTimeout> is an optional timeout value in seconds, with a granularity
 *      of 1/10th of a second. If omitted, INKEY() returns immediately. If set
 *      to 0, INKEY() waits until an input event occurs. If set to any other
 *      value, INKEY() will return either when an input event occurs or when
 *      the timeout period has elapsed. If only this parameter is specified
 *      and it is not numeric, it will be treated as if it were 0. But if both
 *      parameters are specified and this parameter is not numeric, it will be
 *      treated as if it were not present.
 *
 *      <nEvents> is an optional mask of input events that are to be enabled.
 *      If omitted, defaults to hb_set.HB_SET_EVENTMASK. Valid input masks are
 *      in inkey.ch and are explained below. It is recommended that the mask
 *      names be used rather than their numeric values, in case the numeric
 *      values change in future releases of Harbour. To allow more than one
 *      type of input event, simply add the various mask names together.
 *
 *        <table>
 *        inkey.ch            Meaning
 *
 *        INKEY_MOVE          Mouse motion events are allowed
 *        INKEY_LDOWN         The mouse left click down event is allowed
 *        INKEY_LUP           The mouse left click up event is allowed
 *        INKEY_RDOWN         The mouse right click down event is allowed
 *        INKEY_RUP           The mouse right click up event is allowed
 *        INKEY_KEYBOARD      All keyboard events are allowed
 *        INKEY_ALL           All mouse and keyboard events are allowed
 *        HB_INKEY_EXTENDED   Extended keyboard codes are used.
 *        </table>
 *      If the parameter is not numeric, it will be treated as if it were set
 *      to hb_set.HB_SET_EVENTMASK.
 *  $RETURNS$
 *      0 in case of timeout with no input event, otherwise returns a value
 *      in the range -47 to 386 for keyboard events or the range 1001 to 1007
 *      for mouse events. Mouse events and non-printable keyboard events are
 *      represented by the K_<event> values listed in inkey.ch. Keyboard
 *      event return codes in the range 32 through 127 are equivalent to the
 *      printable ASCII character set. Keyboard event return codes in the
 *      range 128 through 255 are assumed to be printable, but results may
 *      vary based on hardware and nationality. If HB_INKEY_EXTENDED mode is
 *      used, then the return value for keyboard events ranges from 1 through
 *      767 and 1077 through 1491, although not all codes are used.
 *
 *      Extended key codes consist of the PC keyboard scan code and one
 *      or more offset values. If no keyboard modifier was used, then
 *      HB_INKEY_NONE is added. The Alt key adds HB_INKEY_ALT, the Ctrl
 *      key adds HB_INKEY_CTRL, the Shift key adds HB_INKEY_SHIFT, and
 *      enhanced keys (KeyPad+/ and CursorPad keys) add HB_INKEY_ENHANCED.
 *      For example, F1 is scan code 59, so if you just press F1, you get
 *      key code 315, but Alt+F1 gives 443, Ctrl+F1 gives 571, and Shift+
 *      F1 gives 699. And NumPad+/ gives 1077, 1205, 1333, and 1461. At
 *      this time, the only value that can combine with other values is
 *      HB_INKEY_ENHANCED (i.e., there are no Alt+Ctl combinations, etc.)
 *
 *      Note: The extended key code set is larger than the normal key code
 *      set. As a result, if you switch between the normal and extended
 *      modes, you need to be aware that some codes get translated into a
 *      zero in normal mode (because there is no corresponding code in
 *      normal mode) and that these codes get removed from the keyboard
 *      input buffer in normal mode and you won't be able to go back and
 *      fetch them later in extended mode.
 *  $DESCRIPTION$
 *      INKEY() can be used to detect input events, such as keypress, mouse
 *      movement, or mouse key clicks (up and/or down).
 *  $EXAMPLES$
 *      // Wait for the user to press the Esc key
 *      ? "Please press the ESC key."
 *      WHILE INKEY( 0.1 ) != K_ESC
 *      END
 *  </fixed>
 *  $TESTS$
 *      KEYBOARD "AB"; ? INKEY(), INKEY() ==>   65   66
 *  </fixed>
 *  $STATUS$
 *      S
 *  $COMPLIANCE$
 *      INKEY() is compliant with the Clipper 5.3 INKEY() function with one
 *      exception: The Harbour INKEY() function will raise an argument error
 *      if the first parameter is less than or equal to 0 and the second
 *      parameter (or the default mask) is not valid, because otherwise INKEY
 *      would never return, because it was, in effect, asked to wait forever
 *      for no events (Note: In Clipper, this also blocks SET KEY events).
 *  $FILES$
 *      Library is rtl
 *  $SEEALSO$
 *      inkey.ch
 *  $END$
 */


/*  $DOC$
 *  $FUNCNAME$
 *      __KEYBOARD()
 *  $CATEGORY$
 *      Console input
 *  $ONELINER$
 *      DO NOT CALL THIS FUNCTION DIRECTLY!
 *  $SYNTAX$
 *      KEYBOARD <cString>
 *      CLEAR TYPEAHEAD
 *  $ARGUMENTS$
 *      <cString> is the optional string to stuff into the Harbour keyboard
 *      buffer after clearing it first. Note: The character ";" is converted
 *      to CHR(13) (this is an undocumented CA-Cl*pper feature).
 *  $RETURNS$
 *      There is no return value.
 *  $DESCRIPTION$
 *      Clears the Harbour keyboard typeahead buffer and then inserts an
 *      optional string into it.
 *  $EXAMPLES$
 *      // Stuff an Enter key into the keyboard buffer
 *      KEYBOARD CHR(13)
 *      // Clear the keyboard buffer
 *      CLEAR TYPEAHEAD
 *  </fixed>
 *  $TESTS$
 *      KEYBOARD CHR(13); ? INKEY() ==> 13
 *      KEYBOARD ";" ? INKEY() ==> 13
 *      KEYBOARD "HELLO"; CLEAR TYPEAHEAD; ? INKEY() ==> 0
 *  </fixed>
 *  $STATUS$
 *      R
 *  $COMPLIANCE$
 *      __KEYBOARD() is compliant with CA-Cl*pper 5.3
 *  $FILES$
 *      Library is rtl
 *  $SEEALSO$
 *    CLEAR TYPEAHEAD,KEYBOARD
 *  $END$
 */

/*  $DOC$
 *  $FUNCNAME$
 *      HB_KEYPUT()
 *  $CATEGORY$
 *      Console input
 *  $ONELINER$
 *      Put an inkey code to the keyboard buffer.
 *  $SYNTAX$
 *      HB_KEYPUT( <nInkeyCode> )
 *  $ARGUMENTS$
 *      <nInkeyCode> is the inkey code, which should be inserted into the
 *      keyboard buffer.
 *  $RETURNS$
 *      There is no return value.
 *  $DESCRIPTION$
 *      Inserts an inkey code to the string buffer. The buffer is *not*
 *      cleared in this operation. This function allows to insert such
 *      inkey codes which are not in the range of 0 to 255. To insert more
 *      than one code, call the function repeatedly. The zero code cannot
 *      be inserted.
 *  $EXAMPLES$
 *      // Stuff an Alt+PgDn key into the keyboard buffer
 *      HB_KEYPUT( K_ALT_PGDN )
 *  </fixed>
 *  $TESTS$
 *      HB_KEYPUT( K_ALT_PGDN ) ; ? INKEY() ==> 417
 *      HB_KEYPUT( K_F11 ) ; ? INKEY() ==> -40
 *  </fixed>
 *  $STATUS$
 *      R
 *  $COMPLIANCE$
 *      HB_KEYPUT() is a Harbour extension.
 *  $FILES$
 *      Library is rtl
 *  $SEEALSO$
 *      KEYBOARD,CLEAR TYPEAHEAD,INKEY()
 *  $END$
 */

/*  $DOC$
 *  $FUNCNAME$
 *      NEXTKEY()
 *  $CATEGORY$
 *      Console input
 *  $ONELINER$
 *      Get the next key code in the buffer without extracting it.
 *  $SYNTAX$
 *      NEXTKEY( [<nInputMask>] ) --> nKey
 *  $ARGUMENTS$
 *      nInputMask is an optional integer value composed of one or more
 *      INKEY_ or HB_INKEY_ constants. The sole purpose of this argument
 *      is to allow switching between using HB_INKEY_EXTENDED key codes
 *      and using the normal Clipper-compatible key codes
 *  $RETURNS$
 *      <nKey>  The value of the next key in the Harbour keyboard buffer.
 *  $DESCRIPTION$
 *      Returns the value of the next key in the Harbour keyboard buffer
 *      without extracting it.
 *  $EXAMPLES$
 *      // Use NEXTKEY() with INKEY() to change display characters, or by
 *      // itself to exit the loop, so that the caller can detect the Esc.
 *      LOCAL nKey, cChar := "+"
 *      WHILE TRUE
 *         ?? cChar
 *         nKey := NEXTKEY()
 *         IF nKey == K_ESC
 *            EXIT
 *         ELSE
 *            IF nKey != 0
 *               cChar := CHR( nKey )
 *            END IF
 *         END IF
 *      END WHILE
 *  </fixed>
 *  $TESTS$
 *      KEYBOARD "AB"; ? NEXTKEY(), NEXTKEY() ==>   65   65
 *  </fixed>
 *  $STATUS$
 *      R
 *  $COMPLIANCE$
 *      NEXTKEY() is compliant with CA-Cl*pper 5.3, but has been extended
 *      for Harbour.
 *  $FILES$
 *      Library is rtl
 *  $SEEALSO$
 *      INKEY(),LASTKEY()
 *  $END$
 */

/*  $DOC$
 *  $FUNCNAME$
 *      LASTKEY()
 *  $CATEGORY$
 *      Console input
 *  $ONELINER$
 *      Get the last key extracted from the keyboard buffer.
 *  $SYNTAX$
 *      LASTKEY( [<nInputMask>] ) --> nKey
 *  $ARGUMENTS$
 *      nInputMask is an optional integer value composed of one or more
 *      INKEY_ or HB_INKEY_ constants. The sole purpose of this argument
 *      is to allow switching between using HB_INKEY_EXTENDED key codes
 *      and using the normal Clipper-compatible key codes
 *  $RETURNS$
 *      <nKey>  The last key extracted from the keyboard buffer.
 *  $DESCRIPTION$
 *      Returns the value of the last key exttracted from the Harbour
 *      keyboard buffer
 *  $EXAMPLES$
 *      // Continue looping unless the ESC key was pressed in MainFunc()
 *      WHILE TRUE
 *         MainFunc()
 *         IF LASTKEY() == K_ESC
 *            EXIT
 *         ENDIF
 *      END WHILE
 *  </fixed>
 *  $TESTS$
 *      KEYBOARD "AB"; ? INKEY(), LASTKEY() ==>   65   65
 *  </fixed>
 *  $STATUS$
 *      R
 *  $COMPLIANCE$
 *      LASTKEY() is compliant with CA-Cl*pper 5.3, but has been extended
 *      for Harbour.
 *  $FILES$
 *      Library is rtl
 *  $SEEALSO$
 *      INKEY(),LASTKEY()
 *  $END$
 */


/*  $DOC$
 *  $FUNCNAME$
 *      KEYBOARD
 *  $CATEGORY$
 *      Command
 *  $ONELINER$
 *      Stuffs the keyboard with a string.
 *  $SYNTAX$
 *      KEYBOARD <cString>
 *  $ARGUMENTS$
 *      <cString> String to be processed, one character at a time,
 *      by the Harbour keyboard processor
 *  $DESCRIPTION$
 *      This command stuffs the input buffer with <cString>. The
 *      number of characters that can be stuffed into the keyboard
 *      buffer is controlled by the SET TYPEAHEAD command and may range
 *      from 0 to 32,622, with each character appearing in the ASCII
 *      range of 0 to 255. None of the extended keys may be stuffed
 *      into the keyboard buffer.
 *      Issuing a KEYBOARD " " will clear the keyboard buffer.
 *  $EXAMPLES$
 *      // Stuff an Enter key into the keyboard buffer
 *      KEYBOARD CHR(13)
 *      // Clear the keyboard buffer
 *      CLEAR TYPEAHEAD
 *  </fixed>
 *  $TESTS$
 *      KEYBOARD CHR(13); ? INKEY() ==> 13
 *      KEYBOARD "HELLO"; CLEAR TYPEAHEAD; ? INKEY() ==> 0
 *  </fixed>
 *  $STATUS$
 *      R
 *  $COMPLIANCE$
 *      __KEYBOARD() is compliant with CA-Cl*pper 5.3
 *  $SEEALSO$
 *       CLEAR TYPEAHEAD,__KEYBOARD()
 *  $END$
 */

/*  $DOC$
 *  $FUNCNAME$
 *      READKEY()*
 *  $CATEGORY$
 *      Data input and output
 *  $ONELINER$
 *      Find out which key terminated a READ.
 *  $SYNTAX$
 *      READKEY() --> nKeyCode
 *  $ARGUMENTS$
 *      None.
 *  $RETURNS$
 *      READKEY() returns a numeric code representing the key that caused READ
 *      to terminate.
 *  $DESCRIPTION$
 *      READKEY() is used after a READ was terminated to determine the exit
 *      key pressed. If the GET buffer was updated during READ, 256 is added
 *      to the return code.
 *
 *      <table>
 *      Exit               Return code     Return code
 *      Key                (not updated)   (updated)

 *      Up                    4            260
 *      Down                  5            261
 *      Page-Up               6            262
 *      Page-Down             7            263
 *      Ctrl Page-Up         34            290
 *      Ctrl Page-Down       35            291
 *      Esc                  12            268
 *      Ctrl End             14            270
 *      Enter                15            271
 *      Key >= 32            15            271
 *      otherwise             0            0
 *      </table>
 *      READKEY() is a compatibility function so try not to use it.
 *      READKEY() is superseded by LASTKEY() which returns the INKEY()
 *      code for that key.  UPDATED() could be used to find if the
 *      GET buffer was changed during the READ.
 *  $STATUS$
 *      R
 *  $COMPLIANCE$
 *      READKEY() is compliant with CA-Cl*pper 5.3
 *  $FILES$
 *      Library is rtl
 *  $SEEALSO$
 *       @...GET,INKEY(),LASTKEY(),READ,READEXIT(),UPDATED()
 *  $END$
 */

/*  $DOC$
 *  $FUNCNAME$
 *      MROW()
 *  $CATEGORY$
 *      Console input
 *  $ONELINER$
 *      Returns the mouse cursor row position.
 *  $SYNTAX$
 *      MRow() --> nMouseRow
 *  $ARGUMENTS$
 *      None
 *  $RETURNS$
 *      <nMouseRow> The mouse cursor row position.
 *  $DESCRIPTION$
 *      This function returns the current mouse row cursor position.
 *      On graphical systems the value represents pixel rows.
 *      On character-based systems the value represents character
 *      rows as in Clipper.
 *  $EXAMPLES$
 *      IF MRow() < 1
 *         ? "Mouse is on top row!"
 *      ENDIF
 *  </fixed>
 *  $STATUS$
 *      R
 *  $COMPLIANCE$
 *      MROW() is compliant with CA-Cl*pper 5.3, but has been extended
 *      to work on graphical systems as well as character-based systems.
 *  $PLATFORMS$
 *  $FILES$
 *      Library is rtl
 *  $SEEALSO$
 *      MCOL()
 *  $END$
 */

/*  $DOC$
 *  $FUNCNAME$
 *      MCOL()
 *  $CATEGORY$
 *      Console input
 *  $ONELINER$
 *      Returns the mouse cursor column position.
 *  $SYNTAX$
 *      MCol() --> nMouseColumn
 *  $ARGUMENTS$
 *      None
 *  $RETURNS$
 *      <nMouseColumn> The mouse cursor column position.
 *  $DESCRIPTION$
 *      This function returns the column position of the mouse cursor.
 *      On graphical systems the value represents pixels.
 *      On character-based systems the value represents character
 *      columns as in Clipper.
 *  $EXAMPLES$
 *      IF MCol() < 1
 *         ? "Mouse is on left edge!"
 *      ENDIF
 *  </fixed>
 *  $STATUS$
 *      R
 *  $COMPLIANCE$
 *      MROW() is compliant with CA-Cl*pper 5.3, but has been extended
 *      to work on graphical systems as well as character-based systems.
 *  $PLATFORMS$
 *      All
 *  $FILES$
 *      Library is rtl
 *  $SEEALSO$
 *      MROW()
 *  $END$
 */
