# Networking FreeDOS - 3Com

      If your 3Com NIC is not supported by the Crynwr packet drivers, you
      can find a driver here:
      ftp://ftp.3com.com/pub/nic/3c90x/3c90x2.exe
      This is EtherCD v5.4, disk 2 of 2 for the 3C90x adapter family. Disk 2
      contains DOS ODI and NDIS drivers, packet driver, help files, and DOS
      diagnostics.  This is a self-extracting DOS executable. After executing
      it, go into the PKTDVR subdirectory, and run 3C90XPD.COM. This should
      auto-detect your NIC, which may take a while, and install the packet
      driver in the first available interrupt vector, starting with 0x60.
      The interrupt vector can also specified with /I; see /? for details.
      You will want to add this to your AUTOEXEC.BAT.
      Afterwards, you can configure and use any WatTCP application, such as
      SSH (see: SSH2DOS) and Arachne. Use this in your WATTCP.CFG to
      specify the interrupt vector:
        pkt.vector = 0x60

#### [Main menu] [top]

      Copyright © 2007 Ulrich Hansen, Mainz (Germany), modified 2010
      by W.Spiegl.
      For more information see here.

      Permission is granted to copy, distribute and/or modify this document
      under the terms of the GNU Free Documentation License, Version 1.1 or
      any later version published by the Free Software Foundation.
      A copy of the license is included in the section entitled
      "GNU Free Documentation License"