# Command: gcdrom.sys

      GCDROM.SYS is a SATA native IDE CD/DVD-ROM driver for DOS
      (aka "ODD DOS driver"). GCDROM.SYS supports all SATA Native IDE
      controller, such as Intel ICH6/ICH7/ICH8, Jmicron 363/368,
      NVidia CK804/MCP55/MCP51 etc.
      GCDROM.SYS has to be loaded in CONFIG.SYS / FDCONFIG.SYS.
      When FreeDOS is already running, you can load GCDROM.SYS later
      with DEVLOAD.
      GCDROM.SYS is out of date. You should use UIDE.SYS instead.

## Syntax:

      device=gcdrom.sys [options]
      devicehigh=gcdrom.sys [options]

#### [Main menu] [top] (Syntax) [Options] [Comments] [Examples] [See also] [File]

## Options:

      /AX  Excludes ALL audio functions. This makes the driver report on a
           Device-Status request that it reads DATA tracks only! /AX reduces
           the resident driver by 448 bytes. UltraDMA, multi-drives, and
           other driver features are NOT affected!
      /Cx  Determines number to detect 1st/2nd/3th SATA native IDE controller.
           Default = 0.
      /D:  Specifies the desired "device name" which SHSUCDX or MSCDEX
           will use during their initialization to address the CD-ROM drives.
           Examples are: /D:CDROM1 /D:MYCDROM etc.
           The device name must be from 1 to 8 bytes valid for use in DOS
           filenames. If /D: is omitted, or the "device name" after
           a /D: is missing or invalid, "XCDROM" will be the default.
      /L   Limits UltraDMA to "low memory" below 640K. /L is REQUIRED to use
           UMBPCI or a similar driver whose upper-memory areas cannot do
           UltraDMA. If /L is given, the driver must load in LOW memory so
           its DMA command-lists can fetch properly, or driver loading will
           ABORT! /L causes any I/O requests above 640K to use "PIO mode"
           input. Note that /L will be IGNORED if /UX is also given.
      /Mn  Specifies the MAXIMUM UltraDMA "mode" to be set for a CD-ROM
           drive, where n is a number between 0 and 6, as follows:
           0 = ATA-16, 16 MB/sec.    4 = ATA-66,   66 MB/sec.
           1 = ATA-25, 25 MB/sec.    5 = ATA-100, 100 MB/sec.
           2 = ATA-33, 33 MB/sec.    6 = ATA-133, 133 MB/sec.
           3 = ATA-44, 44 MB/sec.
           A CD-ROM drive designed to use "modes" LESS than the given value
           will be limited to its own highest "mode". /M will be IGNORED for
           CD-ROM drives which cannot do UltraDMA, and it will be ignored
           for ALL drives if /UX is also given.
      /PM  Requests the driver to check the IDE primary-master unit for a
           CD-ROM drive during driver init. If a CD-ROM drive is NOT found
           as primary-master, driver loading will ABORT!
      /PS  Same as /PM but tests the primary-slave unit only.
      /SM  Same as /PM but tests the secondary-master unit only.
      /SS  Same as /PM but tests the secondary-slave unit only.
           --- NOTE ---
           Using multiple drives, multiple /PM /PS /SM /SS switches can be
           given. The first-specified drive is addressed as "unit 0", the
           second as "unit 1", etc. If fewer switches than drives are given,
           the unreferenced drives will NOT be used. If NO such switches are
           given, the driver "scans" for CD-ROM drives, from primary-master
           to secondary-slave. The first drive found will be "unit 0", the
           second will be "unit 1", etc.
      /UF  Enables "Fast UltraDMA". Data input requests that cross an
           UltraDMA "64K boundary" are executed using a 2-element DMA
           command list, one for data up to the boundary, and one for
           data beyond it. CD-ROM speed is increased significantly. "PIO
           mode" input is still needed for user buffers that are misaligned
           (not at an even 4-byte address). /UF will be IGNORED for CD-ROM
           drives which cannot do UltraDMA.
           --- NOTE ---
           Despite any UltraDMA specs, NOT ALL chipsets or mainboards can
           run multi-element DMA commands properly! Although it is valuable,
           /UF must be TESTED on every system, and "Fast UltraDMA" should
           be enabled with CARE!!
      /UX  Disables ALL UltraDMA, even for CD-ROM drives capable of it. The
           driver then uses "PIO mode" for all data input. /UX should be
           needed only for tests and diagnostic work.
      For each switch, a dash may replace the slash, and lower-case letters
      may be used.

#### [Main menu] [top] [Syntax] (Options) [Comments] [Examples] [See also] [File]

## Comments:

      GCDROM.SYS supports NLS (national language support), see "xcdmsgs.eng".
      It only has to be compiled in the corresponding language.

#### [Main menu] [top] [Syntax] [Options] (Comments) [Examples] [See also] [File]

## Examples:

      IN CONFIG.SYS / FDCONFIG.SYS:
      determine number to detect 1st/2nd/3th SATA native IDE controller:
        DEVICE=c:\fdos\bin\GCDROM.SYS /D:CDROM000 /C0
        DEVICE=c:\fdos\bin\GCDROM.SYS /D:CDROM001 /C1
        DEVICE=c:\fdos\bin\GCDROM.SYS /D:CDROM002 /C2
      IN AUTOEXEC.BAT:
        c:\fdos\bin\SHSUCDX /D:CDROM000 /D:CDROM001 /D:CDROM002

#### [Main menu] [top] [Syntax] [Options] [Comments] (Examples) [See also] [File]

## See also:

     (atapicdd.sys)
      autoexec.bat
      config.sys
      devload
      fdconfig.sys
     (mscdex)
      shsucdx
     (udvd.sys)
      uide.sys
     (xcdrom.sys)

#### [Main menu] [top] [Syntax] [Options] [Comments] [Examples] (See also) [File]

## File:

      Please read this command's lsm file also.
      You will find the updated version (internet) here and
      the version described in this manual page here.
      The lsm file contains information about the name of the programmer,
      the download site, and some other command related information.

#### [Main menu] [top] [Syntax] [Options] [Comments] [Examples] [See also] (File)

      Copyright © 2007 Jack Ellis, updated 2011 by W. Spiegl.

      This file is derived from the FreeDOS Spec Command HOWTO.
      See the file H2Cpying for copying conditions.