# Networking FreeDOS - PKT2ODI

      As an alternative to the more commonly used ODIPKT.COM a few people
      may also like to try out Calderas PKT2ODI.EXE as packet driver to
      ODI converter. But we should be aware, that the license for Novell's
      WebSpyder (which applies to PKT2ODI.EXE) only allows to use the
      software for the purpose of evaluating it. For commercial users the
      evaluation period is restricted to 90 days. For non-commercial users
      evaluation is allowed for "a reasonable period" of time. (Just how
      reasonable can it be to evaluate this software in the 21st century?)
      Anyway, PKT2ODI.EXE will be started in AUTOEXEC.BAT with a command
      like this:
        LH C:\NETWORK\NWCLIENT\PKT2ODI.EXE /B:1 /I:69
      The "/B" option tells PKT2ODI.EXE which logical board it should use.
      Like explained above we have to choose the board that uses the ETHERNET
      II frame. In difference to ODIPKT, PKT2ODI starts counting with "1",
      so if the NET.CFG looks like this example:
        --- NET.CFG ---
          Link Driver 3C574
            FRAME ETHERNET_II
            FRAME ETHERNET_802.2
            FRAME ETHERNET_802.3
            FRAME ETHERNET_SNAP
      we have to use the parameter
        PKT2ODI.EXE /B:1
      to define the use of the first board (the one with ETHERNET_II). Re-
      member that we have to use the board with Ethernet II, otherwise the
      converter won't be able to communicate with the driver and complain
      about not finding the MLID (Multiple Link Interface Driver).

      The second parameter, the "/I" sets the software interrupt (vector)
      used by the driver. We already found out that this should be 0x60, but
      unfortunately this won't work with PKT2ODI. The program doesn't accept
      interrupt vectors 0x60 to 0x68. We may use vector 0x69 with the para-
      meter:
        PKT2ODI.EXE /I:69
      Using an unusual interrupt vector like 0x69 can be a problem for some
      TCP/IP applications. They must be configured to use this vector. Some
      programs, like the webserver SIOUX, may not work correctly, if the
      vector is not 0x60.
      That's all. After starting the LSL (Link Support Layer), the MLID
      (Multiple Link Interface Driver) and the converter the packet driver
      interface should now be up and running.

      (Picture boot messages PKT2ODI)

#### [Main menu] [top] [ODI driver installation]

      Copyright © 2007 Ulrich Hansen, Mainz (Germany), modified 2010
      by W.Spiegl.
      For more information see here.

      Permission is granted to copy, distribute and/or modify this document
      under the terms of the GNU Free Documentation License, Version 1.1 or
      any later version published by the Free Software Foundation.
      A copy of the license is included in the section entitled
      "GNU Free Documentation License"