# Command: graphics-ps, graphpin, graph-hp

      The FreeDOS graphics tool.

## Syntax:

      GRAPH-PS (options) - for laser printers only (PostScript)
      GRAPHPIN (options) - for dot matrix printers and other ESC/P (Epson)
      GRAPH-HP (options) - for HP PCL 3 printers
        I recommend that you copy the file that fits
        YOUR printer to GRAPHICS.COM for better overview.

#### [Main menu] [top] (Syntax) [Options] [Comments] [Examples] [See also] [File]

## Options:

      Common Options:
        /1  Use LPT1 (default)
        /2  Use LPT2
        /3  Use LPT3
        /B  Enable processing of CGA background color 0 palette
        /I  Inverse printing (useful if lots of dark areas on screen, to
            save ink / toner: will print black where screen is white etc.).
        /E  Economy mode: only 50% of the density. Done by reducing the
            distance of every color to white to 50% of the normal value.
        /?  Shows the help screen instead of going resident - you do not
            need to give any options :-)
      Different Options:
      HP (GRAPH-HP - PCL) allows the following extra options:
        /C  For 300 dpi instead of 600 dpi
        /R  Use random dither instead of ordered dither
      PS (GRAPH-PS - Postscript) allows the following extra options:
        /C  Compatibility mode (HP Laserjet)
      PIN (GRAPHPIN - EPSON) allows the following extra options:
        /9  9-pin mode (120x72, with /C 60x72)
        /C  Compatibility mode (120x60dpi)
        /R  Use random dither instead of ordered dither
        /X  Send print data for whole lines instead of in blocks
        After loading the driver you can print screenshots using
        'shift - PrintScreen' even in graphic modes.

#### [Main menu] [top] [Syntax] (Options) [Comments] [Examples] [See also] [File]

## Comments:

    Run the GRAPH*.COM that fits your printer - It will stay resident in
    the background until you reboot. You can use the 'shift PrtScr' key
    while GRAPH... is resident to print hardcopies (screenshots) of your
    graphical screen contents in all standard CGA, EGA and VGA modes.
    No support for high resolution modes / VESA / Hercules yet. The print
    canvas should fit both A4 and letter paper. The screen is printed in
    landscape mode: The bottom of the screen is at the left of the paper.

#### [Main menu] [top] [Syntax] [Options] (Comments) [Examples] [See also] [File]

## Examples:

      graph-ps /1 /e

#### [Main menu] [top] [Syntax] [Options] [Comments] (Examples) [See also] [File]

## See also:

      graphics

#### [Main menu] [top] [Syntax] [Options] [Comments] [Examples] (See also) [File]

## File:

      Please read this command's lsm file also.
      You will find the updated version (internet) here and
      the version described in this manual page here.
      The lsm file contains information about the name of the programmer,
      the download site, and some other command related information.

#### [Main menu] [top] [Syntax] [Options] [Comments] [Examples] [See also] (File)

      Copyright © 2003 Eric Auer, updated 2008 by W. Spiegl.

      This file is derived from the FreeDOS Spec Command HOWTO.
      See the file H2Cpying for copying conditions.