# Netzwerken unter FreeDOS - IPX/SPX

      IPX/SPX steht fuer Internetwork Packet Exchange/Sequenced Packet
      Exchange (Internetarbeit Paketeaustausch/aufeinanderfolgender Pakete-
      austausch). IPX und SPX sind Netzwerkprotokolle, die hauptsaechlich
      in einem Netzwerk verwendet werden, die Novell NetWare Betriebssysteme
      verwenden. Dies ist ein sehr arbeitsspeichereffizientes Protokoll und
      wurde urspruenglich mit dem NIC Treiber kombiniert.
      Mit dem Aufkommen billigeren Arbeitsspeichers und der gestiegenen
      Internetnutzung ist Novell von der Verwendung von IPX/SPX weggegangen
      und verwendet inzwischen stattdessen TCP/IP als Standardprotokoll fuer
      NetWare.

#### [Hauptseite] [oben] [Externe Links]

## Externe Links

        * "Open Data-Link Interface Developer's Guide for NetWare DOS
          Workstation Drivers", Revision A (Novell)
        * ODI Specification: NetWare 16-Bit DOS Protocol Stacks and MLIDs,
          Version 1.03 (Novell), (vgl.: http://developer.novell.com/
          documentation/lancomp/dos_psta/dos_pstack.pdf)
        * Bart's Network Boot Disk ver 2.7 (Bart Lagerweij),
          (vgl.: http://www.nu2.nu/bootdisk/network/)
        * NwDsk: NetWare Boot Disk (IP/IPX) ver 3.25 (Erwin Veermans),
          (vgl.: http://www.veder.com/nwdsk/)

#### [Hauptseite] [oben] (Externe Links)

      Copyright © 2007 Ulrich Hansen, Mainz (Germany), 2010 an die
      FreeDOS-Hilfe angepasst von W.Spiegl.
      Weitergehende Informationen finden Sie hier.

      Permission is granted to copy, distribute and/or modify this document
      under the terms of the GNU Free Documentation License, Version 1.1 or
      any later version published by the Free Software Foundation.
      A copy of the license is included in the section entitled
      "GNU Free Documentation License"