# Networking FreeDOS - IPX/SPX

      IPX/SPX stands for Internetwork Packet Exchange/Sequenced Packet
      Exchange. IPX and SPX are networking protocols used primarily on
      a Network using the Novell NetWare operating systems. This is a
      very memory efficient protocol and was originally combined with
      the NIC driver.
      With the advent of cheaper memory and the explosion of Internet use,
      Novell has moved away from using IPX/SPX and now uses TCP/IP as the
      default protocol for NetWare instead.

#### [Main menu] [top] [External Links]

## External Links

        * "Open Data-Link Interface Developer's Guide for NetWare DOS Work-
          station Drivers", Revision A (Novell)
        * ODI Specification: NetWare 16-Bit DOS Protocol Stacks and MLIDs,
          Version 1.03 (Novell), (see: http://developer.novell.com/
          documentation/lancomp/dos_psta/dos_pstack.pdf)
        * Bart's Network Boot Disk ver 2.7 (Bart Lagerweij),
          (see: http://www.nu2.nu/bootdisk/network/)
        * NwDsk: NetWare Boot Disk (IP/IPX) ver 3.25 (Erwin Veermans),
          (see: http://www.veder.com/nwdsk/)

#### [Main menu] [top] (External Links)

      Copyright © 2007 Ulrich Hansen, Mainz (Germany), modified 2010
      by W.Spiegl.
      For more information see here.

      Permission is granted to copy, distribute and/or modify this document
      under the terms of the GNU Free Documentation License, Version 1.1 or
      any later version published by the Free Software Foundation.
      A copy of the license is included in the section entitled
      "GNU Free Documentation License"