If you are programming with the Waterloo TCP library, the following notes
may prove helpful.

- - -
General Changes                     (7/16/93)
    I did a lot of cleaning up to make this compile more nicely and
    more than a year's worth of bugs have been fixed.

    Several areas underwent protocol optimization to significantly
    improve performance under certain circumstances.  Noticable
    enhancements include SLIP support and fragments reassembly, but
    the latter is currently disabled as I introduced a bug.

- - -
General Changes                     (3/31/92)
    This update has a lot of little bug fixes, optimizations and
    general improvements thanks to a lot of people's input.  In
    particular, Jason Dent and Graham Robinson (author of PKTMUX10).

1. Push bit handling is improved.  This is mostly necessary for 3270
   protocols, most others treat tcp as a simple binary stream.

2. Zero window probing has been fixed.  This will keep things rolling
   even when the remote machine is swamped and the network becomes lossy
   around the same time.

3. A bug in the ASCII tcp stuff was introduced on my site this month
   and has been fixed.  I don't know if the bug was on my old distribution.

4. Significant changes were made to the internal handling of acknowledgements
   and handling data within the receive window.

5. A bug used to annoy SCO and possibly other system consoles - fixed.
   When WATTCP wished to refuse unwanted sessions from remote systems, it
   would be missing a small flag.  Most tcp's didn't notice this flaw.

6. Type of Service flag now RFC compliant - currently unused in non-military
   installations, this flag could be used to set priorities for TELNET
   sessions versus bulk data transfers like FTP, particularly over slow
   lines.  Phil Karn (Mr. KA9Q) is currently researching this area and
   so this upgrade should make WATTCP code react properly (unlike SunOS, BSD,
   etc.) in sites which use his TCPs.

Erick

- - -
Speed/Performance               (1/04/1992)

    The tcp code has undergone some mods to make it much faster, with
    reads up to 120 kilobytes/s and writes up to 42 kilobytes/s on the
    same subnet as my Sun.

    These speed were great, but my pc is usually on a subnet.  There, the
    speeds were about 26 kB/s in writes and 70 kB/s in reads.

    For read's I was able to use good old sock_fastread.  For writes,
    sock_fastwrite / sock_write just don't cut it because they are limited
    to the small buffer size located in the tcp_Socket structure.

    I've added a new call which let's you get around that limitation,
    sock_enqueue().  This new routine let's you specify a buffer of data
    you wish to enqueue for transmission.  WATTCP records the address of
    that buffer and its length, and starts to transmit it according to
    the TCP rules.  You are not allowed to touch that buffer until all
    the data is fully transmitted, something you can tell by using the
    sock_tbused( s ) until it returns zero.  You must also keep calling
    tcp_tick() or sock_tick() as those routines schedule transmissions.


    Here is some sample code which writes out a disk file:

    tcp_open...
    f->dhanle = open( ....
    ...
    while ( 1 ) {
        /* check connection and do background stuff */
        if (tcp_tick( s ) == 0) break;

        /* see if we can schedule more data */
        if ( sock_tbused( s ) == 0 ){
            printf("disk reading %u bytes\n", ftpdbufferlen );
            if ((diff = read( f->dhandle, ftpdbuffer, ftpdbufferlen )) <= 0 ) {
                /* eof or possibly error condition */
                break;
            } else {
                /* data ready to send */
                sock_enqueue( s, ftpdbuffer, diff );
            }
        }
    }

    close( f->dhandle );
    sock_close( s );
- - -
SMTPSERV  (in separate file: SMTPSERV.ZIP)

    This program accepts inbound mail and places it into mail spool files
    almost identically to the way Phil Karn's NOS does.  You can download the
    executable in pub/wattcp/smtpserv.zip.  If you find it useful or wish
    to have it changed, let me know.

-----------------------------------------------------------------------------

Large Model                     (9/13/1991)
    You can compile large or small model applications.  Check out the
    MAKEFILE in the .\APPS subdirectory to see how easy it is to switch.

    The fullsrc.zip collection automatically produces large and small
    model libraries.

    There is a potential problem when you compile applications because
    you make the same mistake I did and place tcp_Socket on the stack
    by declaring it an automatic variable.  The 'C' stack is normally
    only four K, slightly less than the tcp_Socket structure.

    I didn't figure this one out very quickly, so tcp_open, udp_open,
    and tcp_listen have code to warn you immediately and exit in case
    you forget.

-----------------------------------------------------------------------------

TCP Fixes                       (9/13/1991)
     The TCP portion of WATTCP has had numerous improvements.  I've managed
     to significantly reduce the packet count while improving performance
     and reliability.

-----------------------------------------------------------------------------

New Wattcp Programs
     The latest release of MS-Kermit includes the WATTCP kernel, letting you
     use it as a TELNET program.  I do not know where the ftp site is,
     but it will probably be announced soon on Comp.protocols.tcp-ip.ibmpc
     in the near future.

     LPD is a line printer server which will let a PC accept jobs from UNIX.
     It offers some simple device restriction capabilities.  You can spool
     jobs out any DOS file or device.  It requires a little few lines
     of work to be used at any site other than mine.  It is available

     COMD.EXE is a simple program can be used to allow network access to
     RS232 devices.  With a little work it could be converted into a modem
     pool.  It is available from [129.97.128.196] pub/wattcp/comd.zip.

     If you have any improvements or new applications, please let me know.
     I will gladly distribute them for you.

-----------------------------------------------------------------------------

Nested Config Files             (7/16/91)
    Wattcp config files may be easily nested to allow for centralized
    control of most parameters with local overrides, or user specific
    extensions.

    To include a nested config file, use the following line in the
    main config file:

        include = filename
    eg. include = c:\local.cfg

    If the local file could not be found, a warning message is displayed.
    You may wish to use a local file if it exists, but not display a message
    if it does not.  To do that, simply prepend the filename with a question
    mark.

    eg. include = ?c:\local.cfg

    When the nested file is complete it will return to the main file.

    The nesting limit is dependant upon the number of unused file handles
    and the stack size.

-----------------------------------------------------------------------------

TCP/UDP Packet Dumps            (7/10/1991)
    TCP/UDP packet dumping features have been added and may prove useful
    for testing and debugging your applications.

    The debugger dumps packets, which gives you a feel for what the
    kernal and the other end are trying to do.

    It's my job to try to make things go as fast as possible with as
    few packets as possible (least load).  Actually, when you use the
    dumping feature you usually INCREASE the packet count because the
    dumper takes time which times out the scheduler and causes
    retransmits.

    To include the debugging features in your program, add the line
        dbuginit();
    to your program *before* you call sock_init();

    To enable/disable the debugger, include the following lines in your
    WATTCP.CFG file:
        DEBUG.FILE=somename     # otherwise it will open a file called
                                # WATTCP.DBG in the current subdirectory
                                # somename could be con which will dump
                                # to the screen
        DEBUG.MODE=DUMP         # to dump TCP/UDP data, looks a bit like
                                # DEBUG.COM
   or   DEBUG.MODE=HEADERS      # to dump TCP/UDP headers
   or   DEBUG.MODE=ALL          # to dump everything, headers and data

   You may write some textual data directly to the file.  Remember, you
   must send a 'C' string ending with a 0, and you must include your
   own CRLFs.

        db_write( char *msg );

   NOTE: If you use this feature and you also use usr_init, you
         must chain usr_init as described in the programmers manual,
         and as show in TCPINFO.C.

-----------------------------------------------------------------------------
Good UDP Support                (6/5/1991)
   Initially, only standard socket calls could be used for UDP.  That was kind
   of shabby because UDP tends to be higher traffic, has no flow control, and
   you wish to know record boundaries.

   The new code allows you to declare a big buffer into which the incomming
   UDP packets will be bufferred.  Once initialized with sock_recv_init, the
   buffer is used until the socket is closed.  NOTE: sock_recv... and the
   regular socket input routines are MUTUALLY EXCLUSIVE, you can not use
   one and the other at the same time.  

        byte bigbuf[ 8192 ];
        byte smallbuf[ 512 ];
        int templen;

        if ( !udp_open( &data, localport, remote, remoteport, NULL) ) {
            printf("Error opening UDP channel");
            exit( 3 );
        }
        /* set the big buffer */
        if ( sock_recv_init( &data, bigbuf, sizeof( bigbuf )) == -1 ) {
            printf("Error setting the receive buffers");
            exit( 3 );
        }
        while ( 1 ) {
            tcp_tick( NULL );           /* got to do this or sock_tick */

            /* check for incomming udp data */
            if ( templen = sock_recv( &data, smallbuf, sizeof( smallbuf ))) {
                /* something received and it was templen bytes long */
            }
        }
        sock_Close( &data );

   sock_recv... adds extra code, so it need not be used for simple UDP sockets
   such as BOOTP which expects only a single packet.

   See sock_mode checksums below for more interesting notes.

-----------------------------------------------------------------------------
UDP Checksums                   (6/5/1991)
   sock_mode can be used to enable or disable checksums for udp sessions
   using the following calls:

        sock_mode( &socket, UDP_MODE_CHK );
        sock_mode( &socket, UDP_MODE_NOCHK );

   Unlike *some* systems, Waterloo TCP correctly assumes checksums are active
   and allows an application to disable them on the fly as they consider
   appropriate.

   Either or both sides may disable or re-enable checksums.

-----------------------------------------------------------------------------
TCP Nagle Algorithm             (6/5/1991)
   The Nagle algorithm is now used to collect data.  Nagle is ideally suited
   to programs like TELNET (TCPPORT), etc. which send a lot of small chunks
   of data.  Some programs, like X-Windows, real-time data collection, etc.,
   should turn of the Nagle feature.  Nagle is on by default and should not
   be disabled unless a true problem is experienced.

        sock_mode( &socket, TCP_MODE_NONAGLE ); /* turns it off */
        sock_mode( &socket, TCP_MODE_NAGLE );   /* re-enables it */

-----------------------------------------------------------------------------
getdomainname Changes           (6/5/1991)
   getdomainname always took a string and length parameter, just like UNIX.
   Now, if the length is zero, getdomainname just returns the pointer to
   a system copy of the domainstring.

-----------------------------------------------------------------------------
gethostname sethostname Changes (6/5/1991)
   gethostname and sethostname are now available.  They work identically to
   get/setdomainname() (as enhanced above).  The host name can either be set
   via the WATTCP.CFG file or via bootp.
-----------------------------------------------------------------------------

sock_PreRead addition           (4/26/1991)

   int sock_PreRead( void *s, byte *dp, int len );

   Some situations arise where it would be nice to read data without causing
   it to disappear from the socket's buffer.  Usually that means double
   buffering.  sock_PreRead works exactly like sock_FastRead, except it does
   not remove the read data from the data buffers.  The returned value is the
   number of bytes transferred, 0 for no data waiting, or -1 on a socket
   error.

   This function is intended for special cases which are not easily performed
   using other methods.

-----------------------------------------------------------------------------

sethostid addition              (4/26/1991)

   longword sethostid( longword ip );

   This function sets the system's default ip address.  Changing the ip address
   will destroy existing TCP and UDP sessions.  You should close all sockets
   before calling this function.  The passed ip address is always returned.

   This function is low level and rarely useful to an application programmer.

   main()
   {
       longword ip = 0x80010101;   /* 128.1.1.1 */
       char buffer[ 512 ];

       sock_init();
       sethostid( ip );
       printf("IP address has been set to %s\n\r",
           inet_ntoa( buffer, getipaddr() );
   }

-----------------------------------------------------------------------------

setdomainname addition          (4/26/1991)

   char *setdomainname( char *string);

   The domain name returned by getdomainname and used for resolve() is set to
   the value in the string passed to setdomainname().  Note that changing the
   contents of the string after a setdomainname() call may or may not change
   the value of the system domain string and is not recommended.  You are
   recommended to dedicate a static location which will permanently hold that
   name.

   setdomainname( NULL ) is an acceptable way to totally remove any domain name
   and subsequently resolves will not attempt to append a domain name.

   The passed string is always returned, as demonstrated below.

   This function is low level and rarely useful to an application programmer.

   #include <stdio.h>
   #include <tcp.h>
   char buffer[ 512 ];  /* use a static or a calloc, do not place the name
                           in a local variable on the stack, it may get lost! */
   main()
   {
       sock_init();
       puts("Enter a new domain");
       gets( buffer );
       printf("Was using %s\n\r", getdomainname());
       printf("Now using %s\n\r", setdomainname( buffer ));

       setdomainname( NULL );
       puts("Now using no domain name");
   }

-----------------------------------------------------------------------------

_arp_resolve addition           (4/26/1991)

   _arp_resolve( longword ina, void *ethap)

   Given an ip address (ina), find the hardware address.  If ethap is non-NULL,
   place the hardware address in the buffer pointed to by ethap.

   Each call to _arp_resolve checks a local cache to see if we already know
   the hardware address.  If no entry exists for that IP address, steps
   are taken to find a hardware address.  If the ip node is on our subnet,
   an ARP request is broadcast, otherwise _arp_resolve is called recursively
   to find the address to the gateway.

   Socket opens intrinsically call _arp_resolve and place the hardware address
   in the socket structure so they are no longer dependant upon existance in
   the cache.  This means existing tcp and udp sessions do not automatically
   reconfigure if a new route is found to the remote host, but this is typical
   of pc implementations and is quite reasonable.

   Programs which wish to force the hardware address to be in the arp cache
   need only specify the ip address and NULL for the ethap buffer.

   Returns 1 on success or 0 if the ip address could not be resolved.

   This is a special use function and is rarely necessary for user
   applications.

-----------------------------------------------------------------------------

