2004/10/28: (v2.2.alpha.01)

new...
. RAIDWatch: Out-band supports MacOS X
. RAIDWatch: Modify login interface
. RAIDWatch: Add "Strip Size" field in LD information table.
. RAIDWatch: New function: "Restoring Configuration from XML File" at Configuration List.
. RAIDWatch: SATA Drive Channel supports SMART functions.
. RAIDWatch, Configuration Client: Support japanese online help.

bugs...
. Configuration Client: Tooltip in service status, online & offline wrong display.

=====================================================================

2004/11/18: (v2.2.alpha.02)

new...
. RAIDWatch: New function  "Continue adding SCSI drives " while the adding 
             drive operation was paused by Rebuild LD.
. RAIDWatch: Remove the "Lun Map Filter" related informations and functions.

=====================================================================

2004/12/03: (v2.2.alpha.03)

new...
. RAIDWatch: New function  
             (1) "Restore factory defaults" in item "Drive-side parameters"
             (2) Store "User configure information" in host side computer 
                 for RAIDWatch Application mode
. RAIDWatch: suport models "A16F-R2221" & "F16F-R2021-6" 

=====================================================================

2004/12/07: (v2.2.alpha.04)

fixed bugs...
. RAIDWatch:  Use borwer to open RAIDwatch, browser fail;
. RAIDWatch:  Select what's this or Help topic items on Help, those doesn't appear content 

=====================================================================

2004/12/14: (v2.2.alpha.05)

new...
. RAIDWatch Gate application.
. RAIDWatch: New incomming events in RAIDWatch will blink.

fixed bug...
. RAIDWatch: support model "A16F-R2221"

=====================================================================

2005/1/5: (v2.2.alpha.06)

new...
. RAIDWatch: Multi-Language support Deutsch.
. RAIDWatch: RAIDWatch uninstaller can change the components to remove.

=====================================================================

2005/01/27: (v2.2.alpha.07)

new...
. RAIDWatch: Quick Installation in System Menu Bar
. RW Installshield: New installation step can help user to chose basic or advanced installation items
. RAIDWatch: Scan disk for SCSI drive

=====================================================================

2005/02/16: (v2.2.alpha.08)
 
fixed bug...
. RAIDWatch: While asign local spare drive to a RAID 5 LD, if local spare drive's size is smaller 
             than the LD, it will show "SCSI Drive size is too small"
. RAIDWatch: If shutdown the controller, then we can choose to reset controller or not
. RAIDWatch: Fix the Com port Baud Rate displays error value

=====================================================================

2005/02/25: (v2.2.alpha.09) 

new...
. RAIDWatch: Key-in IP Address with "Auto-Complete " function in RaidWatch Login
. RAIDWatch: Configuration List can solely output the host Lun list as XML file.

=====================================================================
2005/03/14: (v2.2.alpha.10) 

new...
. RAIDWatch: Quick Installation function in RAIDWatch -> Configuration 

=====================================================================
2005/03/18: (v2.2.alpha.11) 

new...
. Installshield : The step "basic install" and "advanced install" renamed
                  "typical" and "custom". "Typical" type can choose the 
                  Destination folder to install RAIDWatch.
. Configure: In sub-system mode, controller neednot been restart after setting 
             the on-board npc configuration.

remove...
. RAIDWatch Gate application.
. Uninstallshield: Can not choose the installed components to remove.

=====================================================================
2005/03/29: (v2.2.alpha.12) 

new...
. Installshield: Raid Agent would be installed while choosing "Typical Mode".  

. RAIDWatch: Host Lun filter in Lun Map Sheet.

=====================================================================
2005/03/31: (v2.2.alpha.13) 

new...
. RAIDWatch: Scan disk for SCSI device in Physical Drives => function 
. RAIDWatch: Delete spare drive in Physical Drives => function

=====================================================================
2005/04/08: (v2.2.alpha.14) 

fixed bugs...
(1)Enclosure view => WD 2500SD drive speed show 152 MB but Terminal show 150 MB
(2)Configuration Parameters => other =>Maximum Drive Response Timout(ms) =>The value different from Configuration list => Maximum Drive Response Timout(ms)
(3)In the Configuraiton parameter-->setting disk array parameter -->Maximum Drive Response Timeout 640(ms),but in the Configuraiton List is show 320(ms) 
(4)Problems with customization
(5)Task Schedules => add a new Schedules  Task =>The work finish =>The item can't  auto disappear
(6)make shutdown controller, if press Yes for shutdown controller and then reset, then will not display "reset completed" on RW when controller reseting.
(7)In NPC, When we setting the Auto Discovery then will have the many root-agent,but we want to delete it just can delete one by one,can not select all to delete

=====================================================================
2005/04/12: (v2.2.alpha.15) 

fixed bugs...
(1)Subsystem mode does support Auto Discovery, but still was allowed to press "system / Auto Discovery".
(2)Subsystem Mode: Configure.htm, Boardcast function. Add Broadcast Receive's Host name, But the Title is different: Left side show "Host IP", Right side show "Host name".
(3)When the copy and replace drive capacity is smaller than source drive ,RW will show "Copy and Replace command Fail" but Terminal will show "Select Drive Capacity too small"
(4)Found if the LD is in adding Drive progress,then to do Rebuilding or regenerate parity can not abort the task under Tasks process of rebuilding or regenerate parity
(5)Create a LV then In configuration list --> in the LV setting will have the "assigment-Primary controller",But this is single model
(6)Use Information mode enter RW,In configuration list,Press mouse right button then click "Restore configuration from XML file",if we give it a different configure XML file,It will restore pass and change the configure(Information mode just can view)

=====================================================================
2005/04/18: (v2.2.alpha.16) 

fixed bugs...
(1)If SSL enable, then RW connected with controller via outband then view event log that is empty.
(2)Event log list problems in Redundant mode
(3)Multi -Language supports
(4)set Date/Time then apply, the RW will shows message "change this setting will not take effect until the controller is RESET", but RS232 hasn't show that.
(5)Controller UID Auto Discovery got "0". 
(6)Use Auto Discovery  Connect RW, RW will pop_up the information " Connect failed! Maybe the password is wrong, input the password again, please"
(7)on solaris, when install RW and select custom install, then view destination folder disappear
(8)first RW has connected six connection, then when RW connecting 7th connection the RW halt on initialing and java command shows "out of memory error".
(9)RaidWatch v2.0.c connection, RaidWatch connect overnight, about 4hrs later RaidWatch connect failed
(10)Under Mac OS X (Traditional Chinese),After install the RW finish then click RAIDwatch icon to open RAIDwatch, but can not use the RW application no respond
(11)RaidWatch v2.0.c or v2.2.alpha15, SATA2 Hitachi 3GHz drive,  physical driver speed show "320MB".( FW is 300MB)
(12)SATA2 drive on 266 or cube controller, the Channel (driver channel) / default Data Rate does not have 3.0GHz options.

=====================================================================
2005/04/22: (v2.2.A.01)

fixed bugs...

Configure: Configure.htm settting upload fail.
RAIDWatch: Password error message tuned
RAIDWatch: Multiple -Sessions Memory allocation problem.

=====================================================================
2005/05/03: (v2.2.a.02)

New support models...

RAIDWatch: U16U-G4020
           A24U-G2421
           A24F-R2224

=====================================================================
2005/05/09: (v2.2.a.03)

fixed bugs...

Configure: Configure.htm / SNMP function fail, if input non-number word , will cause event log blank. 
RAIDWatch: Select "cache dirty" or "disk Read / write pergormance" items , Raid watch  hang up.

=====================================================================
2005/05/11: (v2.2.a.04)

fixed bugs...

Configuration Client: Disabled Fax and SMS in Mac OS.
RAIDWatch: Scan SCSI drive error .
RAIDWatch: Help Topic error in Windows2000 AS platform. 
RAIDWatch: Root Agent list IP display error after controller reset.

=====================================================================
2005/06/03: (v2.2.b.01)

new...
Configuration Client: Connect to RootAgent set timeout 5 sec, and alert timeout message.

fixed bugs...
RAIDWatch: Model (F16F-R/S2021-6) Fail PSU fan 0 =>fan 1 LED show red but fan 0 LED show green
RAIDWatch: In configuration menu channel panel pressd refash, this channel list will disappear
RAIDWatch: Fibre JBOD (JBOD-ESF16F-16-I) drive slot position changed.

=====================================================================
2005/06/08: (v2.2.b.02)

fixed bugs..
RAIDWatch: Pull down menu for view/edit LD under "Existing Logical Drive menu".
RAIDWatch: Pull down menu for view/edit LV under "Existing Logical Volumn menu". 
RAIDWatch: Pull down menu for add/remove map under "Host Lun Mapping menu".
RAIDWatch: Goto web button function fail in MacOS platform.
RAIDWatch: The channel(channel type: SATA, mode:RCC ) data rate can be modified, 
           if data rate changed , controller will hung .

===================================================================== 
2005/06/14: (v2.2.b.03)

fixed bugs..

Configuration Client: Lost the Fax and SMS items.

RAIDWatch: Download FW 3.42H05 via RW, RW display "Download FW fail". Actually the download progress is OK.
RAIDWatch: Model A24UG2421 has no BBU led. 
RAIDWatch: In front view, drive speed show 21MB, but terminal show 150MB.
           
===================================================================== 
2005/06/15: (v2.2.b.04)

fixed bugs..

RAIDWatch: Download FW 3.42H05 via RW inband, RW display "Download FW fail".
RAIDWatch: Config controller name can't over 20 characters.
           
===================================================================== 
2005/06/16: (v2.2.b.05)

fixed bugs..

RAIDWatch: Can not login F16F-R2021-6, A24U-G2421.

===================================================================== 

2005/06/17: (v2.2.b.06)

fixed bugs..

RAIDWatch: Download FW and Bootrecord via RW inband, RW display "Download FW fail".
RAIDWatch: Inband controller name can't over 20 characters. 

===================================================================== 

2005/06/24: (v2.2.b.07)

fixed bugs..

RAIDWatch: Under Linux 9, F16F-R2021-6 connect to Fibre Jbod, Jbod sometimes disappeared.
RAIDWatch: Under Linux9 Inband connection to F16F-R2021-6 for a long time (+JBOD)

===================================================================== 
 
2005/07/29: (v2.2.c.01)

new...
. RAIDWatch: RAID 6
. RAIDWatch: LD Migration
. RAIDWatch: Support AV optimization in "Disk-array parameters" panel.
. RAIDWatch: Support Maximum HDD response time on write in "Disk-array parameters" panel. 
. RAIDWatch: Support 512/1024 KB stripe size option
. RAIDWatch: Drive-spin down for SATA/SAS drive in "Drive-side parameters" panel.
. RAIDWatch: Cross-controller LD access (in LD creation panel). 
. RAIDWatch: User configurable drive side cache "Enable" or "Disable" in "Drive-side parameters" panel (only for SATA drive).
. RAIDWatch: Privide different option to let user select if he wants to restore password or not.
. RAIDWatch: Disable rolling firmware upgrade 
. RAIDWatch: Support new models: A16F-G2422, A16F-R2422, A16F-S2422, ESFF-R2021, ESFF-S2021


fixed bug
. Configuration Client: Root-agent support 20 chars password. 

===================================================================== 

2005/08/03: (v2.2.c.02)

fixed bugs

. RAIDWatch: RAID 1, RAID 3 logical drive migrate.
. RAIDWatch: Support fibre 4G
. RAIDWatch: Rearview disappeared
. RAIDWatch: Restore NVRAM with password UI bug.
. RAIDWatch: In-band connect fail.
. RAIDWatch: Download firmware and rolling firmware upgrade UI bug.

===================================================================== 

2005/08/09: (v2.2.c.03)

fixed bugs

. RAIDWatch: RAID 1, RAID 3 logical drive migrate.
. RAIDWatch: LD in online-initial state and regenerate parity, can do rebuild
. RAIDWatch: LD in online-initial state can abort
. RAIDWatch: LD in online-initial state can do media scan
. RAIDWatch: Download firmware bootrecord without reset completed message.
. RAIDWatch: Fail one LD's member drive and can do media scan and migrate
. RAIDWatch: In rebuilding state and the LD can do regerate parity.
. RAIDWatch: On-line initialization and Off-line initialization status error
. RAIDWatch: Expanding status error
. RAIDWatch: Can't assign spare drive. 

===================================================================== 
 
2005/08/12: (v2.2.c.04)

 Fixed bugs...

. RAIDWatch: In-band operation failed in Linux platform.
. RAIDWatch: LD in online-initial state can do expand and migrate LD
. RAIDWatch: Partition UI display abnormal while LV expanding
. RAIDWatch: Quick install Raid 3 LD make RAIDWatch UI display abnormal
. RAIDWatch: RW spindown idle delay items different from Terminal UI
. RAIDWatch: Host Lun Map Filter item disappear
. RAIDWatch: Mode ESFF-S2021 not support  
 
 Remove...
. RAIDWatch: AV optimization item

===================================================================== 
 
2005/08/19: (v2.2.c.05)

 Fixed bugs...
. RAIDWatch: Can't differentiate between "Add Drive" and "Migration"
. RAIDWatch: "Spindown idle delay" UI display abnormal in configuration list
. RAIDWatch: Host lun filter "access mode" UI display abnormal 
. RAIDWatch: Host lun filter "id mask" UI display abnormal 
. RAIDWatch: LD can execute media scan and rebuild while adding drives or migrating LDs.
. RAIDWatch: RW will hang if it doesn't successfully scan fail drive and user rebuild the fail drive
. RAIDWatch: Can't add spare drive. 

. Confugure: Setting complete and upload configuration file will make controller occur unrecoverable error.
 
New...
. RAIDWatch: AV optimization 
. RAIDWatch: bad block reassignment 
. RAIDWatch: Support Models: A24U-G2426-1 , A24F-R2226

===================================================================== 
 
2005/08/24: (v2.2.c.06)

 Fixed bugs...
. RAIDWatch: Problems with delete and add spare drive
. RAIDWatch: Can't assign controller while creating LV
. RAIDWatch: Can't config all items in disk-array parameter panel
. RAIDWatch: Host lun filter UI displays abnormal after create LDs


===================================================================== 

2005/08/29: (v2.2.c.07)

.RAIDWatch: A24U-G2426-1 -change model name into A24U-G2421-1 
.RAIDWatch: A24F-R2226 - change model name to A24F-R2224-1


===================================================================== 
 
2005/08/31: (v2.2.c.08)

new 
.RAIDWatch
.Configure

Created a new certificate in "RAIDWatch and Configure.htm" and it will expire in 2050.

===================================================================== 
 
2005/09/02: (v2.2.c.09)

Fixed bugs... 
. RAIDWatch: Can't config all items in disk-array parameter panel
. RAIDWatch: The certificate on RW 2.2.c subsystem mode is expired on 24 March 05. I have removed the on-line help in subsystem mode.

new ...
. RAIDWatch On-line Help

Modified the following pages:
  - new_features.htm
  - host_drive.htm
  - other.htm
  - adding.htm
  - create_LD.htm
  - RAID_levels.htm
  - system.htm

and added one page:
  - Migration_LD.htm

===================================================================== 
 
2005/09/06: (v2.2.c.10)

Fixed bugs... 
. RAIDWatch: After perpetual clone from one logical drive's member, 
             we can't clone another member with global spare.
. RAIDWatch: In model FF-R2021, drive slot information is wrong.

===================================================================== 
 
2005/09/06: (v2.2.c.11)


Fixed bugs... 
. RAIDWatch: Can't choose the installation floder in Solaris 9
. RAIDWatch: Assign global spare to clone, even if it has local spare,
             it finished but using local spare. 
	     RW change the clone procedure by remove the step "choose targe drive".
. RAIDWatch: The Apply button in configure->other panel disappeared.

===================================================================== 
 
2005/09/07: (v2.2.c.12)


Remove... 
. RAIDWatch: Bad Block Reassignment Threshold
