Login to Road Runner

- Configure ZyAIR to login Road Runner cable ISP

Most settings of connecting to Internet are the same with the guide introduced in the Internet Connection page, this guide will only introduce the extra settings for loging to Road Runner cable ISP in US.

1. Enter Menu 4 from SMT

`Menu 4 - Internet Access Setup ISP's Name= R-Runner Encapsulation= Ethernet Service Type= RR-Manager My Login= myusername My Password= ******** Retype to Confirm= N/A Login Server= 204.210.7.45 Relogin Every (min)= N/A IP Address Assignment= Dynamic IP Address= N/A IP Subnet Mask= N/A Gateway IP Address= N/A Network Address Translation= SUA Only`

Key settings:

- Service Type.......Currently, there are two authentication types that Road Runner supports, RoadRunner and RR-Manager. Choose the correct one for your local ISP.
- Server IP.............The ZyAIR will find the Road Runner server IP if this field is blank, otherwise enter the authentication server IP address if you know it.
- My Login Name...Enter the login name given to you by your ISP
- My Password.......Enter the password associated with the login name
- WAN IP Address Assignment...If the ISP did not assign you an explicit IP, select Dynamic, otherwise, select Static.
- IP Address & Subnet Mask & Gateway IP Address...Enter the IP address & subnet mask & gateway IP when Static Assignment is select above.

All contents copyright © 2004 ZyXEL Communications Corporation.