CI command List

Command Class List Table
System Related Command | Exit Command | Ethernet Related Command
Wireless LAN Related Command | IP Related Command | Bridge Related Command
802.1x Related Command |  |

CI Command List

System Related Command

SYS

Command | Description
sys |  |  |  |
| adjtime |  |  | retrive date and time from Internet
| callhist |  |  |
|  | display |  | display call history
|  | remove | <index> | remove entry from call history
| countrycode |  | [countrycode] | set country code
| date |  | [year month date] | set/display date
| domainname |  |  | display domain name
| edit |  | <filename> | edit a text file
| extraphnum |  |  | maintain extra phone numbers for outcalls
|  | add | <set 1-3> <1st phone num> [2nd phone num] | add extra phone numbers
|  | display |  | display extra phone numbers
|  | node | <num> | set all extend phone number to remote node <num>
|  | remove | <set 1-3> | remove extra phone numbers
|  | reset |  | reset flag and mask
| feature |  |  | display feature bit
| hostname |  | [hostname] | display system hostname
| log |  |  |
|  | clear |  | clear log error
|  | disp |  | display log error
|  | online | [on|off] | turn on/off error log online display
| rn |  |  |
|  | load | <entry no.> | load remote node information
|  | disp | <entry no.>(0:working buffer) | display remote node information
|  | nat | <none|sua|full_feature> | config remote node nat
|  | nailup | <no|yes> | config remote node nailup
|  | save | [entry no.] | save remote node information
| stdio |  | [second] | change terminal timeout value
| systemname |  | [system name] | Change system name
| time |  | [hour [min [sec]]] | display/set system time
| trcdisp | parse, brief, disp |  | monitor packets
| trclog |  |  |
| trcpacket |  |  |
| syslog |  |  |
|  | server | [destIP] | set syslog server IP address
|  | facility | <FacilityNo> | set syslog facility
|  | type | [type] | set/display syslog type flag
|  | mode | [on|off] | set syslog mode
| version |  |  | display RAS code and driver version
| view |  | <filename> | view a text file
| wdog |  |  |
|  | switch | [on|off] | set on/off wdog
|  | cnt | [value] | display watchdog counts value: 0-34463
| romreset |  |  | restore default romfile
| socket |  |  | display system socket information
| filter |  |  |
|  | netbios |  |
| cpu |  |  |
|  | display |  | display CPU utilization

Exit Command

Exit

Command | Description
exit |  |  |  | exit smt menu

Ethernet Related Command

Ether

Command | Description
ether |  |  |  |
| config |  |  | display LAN configuration information
| driver |  |  |
|  | cnt |  |
|  |  | disp <name> | display ether driver counters
|  | ioctl | <ch_name> | Useless in this stage.
|  | status | <ch_name> | see LAN status
| version |  |  | see ethernet device type
| edit |  |  |
|  | load | <ether no.> | load ether data from spt
|  | save |  | save ether data to spt

Wireless LAN Related Command

wlan

Command | Description
wlan |  |  |  |
| active |  | [on|off] | set on/off wlan
| association |  |  | display association list
| chid |  | [channel id] | set channel
| diagnose |  |  | self-diagnostics
| essid |  | [ess id] | set ESS ID
| scan |  |  | scan wireless channels
| version |  |  | display WLAN version information

IP Related Command

ip

Command | Description
ip |  |  |  |
| address |  | [addr] | display host ip address
| arp |  |  |
|  | status | <iface> | display ip arp status
| dhcp |  | <iface> |
|  | client |  |
|  |  | release | release DHCP client IP
|  |  | renew | renew DHCP client IP
|  | status | [option] | show dhcp status
| dns |  |  |
|  | query |  |
|  | stats |  |
| httpd |  |  |
| icmp |  |  |
|  | status |  | display icmp statistic counter
|  | discovery | <iface> [on|off] | set icmp router discovery flag
| ifconfig |  | [iface] [ipaddr] [broadcast <addr> |mtu <value>|dynamic] | configure network interface
| ping |  | <hostid> | ping remote host
| route |  |  |
|  | status | [if] | display routing table
|  | add | <dest_addr|default>[/<bits>] <gateway> [<metric>] | add route
|  | addiface | <dest_addr|default>[/<bits>] <gateway> [<metric>] | add an entry to the routing table to iface
|  | addprivate | <dest_addr|default>[/<bits>] <gateway> [<metric>] | add private route
|  | drop | <host addr> [/<bits>] | drop a route
| status |  |  | display ip statistic counters
| udp |  |  |
|  | status |  | display udp status
| rip |  |  |
| tcp |  |  |
|  | status | [tcb] [<interval>] | display TCP statistic counters
| telnet |  | <host> [port] | execute telnet clinet command
| tftp |  |  |
| traceroute |  | <host> [ttl] [wait] [queries] | send probes to trace route of a remote host
| xparent |  |  |
|  | join | <iface1> [<iface2>] | join iface2 to iface1 group
|  | break | <iface> | break iface to leave ipxparent group

Bridge Related Command

Bridge

Command | Description
Bridge |  |  |  |
| cnt |  |  | related to bridge routing statistic table
|  | disp |  | display bridge route counter
|  | clear |  | clear bridge route counter
| stat |  |  | related to bridge packet statistic table
|  | disp |  | display bridge route packet counter
|  | clear |  | clear bridge route packet counter

802.1x Related Command

8021x

Command | Description
8021x |  |  |  |
| radius | authentication | Show | show current radius authentication server configuration
|  | accounting | Show | show current radius accounting server configuration
| debug | reauth | <0:off 1:on> | set IEEE802.1x reauthentication method
|  | level | [debug level] | set ieee802.1x debug message level
|  | trace |  | show all supplications in the supplication table
|  | user | [username] | show the specified user status in the supplicant table

All contents copyright (c) 2003 ZyXEL Communications Corporation.