Setup the ZyAIR for PPPoE Connections

- Introduction

PPP over Ethernet is an IETF draft standard specifying how a host personal computer (PC) interacts with a broadband modem (i.e. xDSL, cable etc.) to achieve access to the high-speed data networks via a familiar PPP dialer such as 'Dial-Up Networking' user interface. PPPoE supports a broad range of existing applications and service including authentication, accounting, secure access and configuration management. There are several major service providers running evaluations of PPPoE today. Before using PPPoE feature of the ZyWALL, please make sure your ISP supports PPPoE.

- Setup the ZyAIR for Internet Access using PPPoE

1. Configure PPPoE Assignment in Web GUI -> WAN/LAN -> WAN Port mode ->PPPoE

2. Type the Username and Password for making a PPPoE connection.

3. Click Apply to finish.

All contents copyright (c) 2004 ZyXEL Communications Corporation.