Setting Up the Syslog Facility

What is the ZyAIR syslog facility?

The ZyAIR's syslog function allows network administrator to monitor the usage status of subscribers from a remote site. You can set up a sys log server to receive the log of information on current logged in subscribers that the ZyAIR send periodically.

- Configure the settings of the syslog server

- Configure the settings of the syslog server

Configuration:

1. Select Enable in the syslog option to activate the Syslog function.

2. Select the check box to specify a syslog server on the LAN (or WAN).

3. Enter the IP address (in dotted decimal notation) of the syslog server on the LAN (or WAN).

4. Enter the MAC address of the syslog server on the LAN (or WAN).

5. Click Apply to save the settings.

6. Use the Syslog log settings screen to configure which logs the ZyAIR is to send.

7. Select the check box you need to send the log information to your syslog server.

8. Click Apply to save the settings.

All contents copyright © 2004 ZyXEL Communications Corporation.