Upgrade firmware using Web configurator

The ZyAIR embedded Web configurator to upgrade firmware. To manually upgrade the the firmware, you have to go to download the latest firmware first from www.zyxel.com and then upload it to the ZyAIR.

Upgrading a software file

- 1. Download the default firmware file from the ZyXEL ftp server, unzip it and save it in a folder.
- 2. Select System tool in the ZyAIR Web configurator and click FIRMWARE. Select the unzipped file in your Local PC File Path.
- 3. Click Apply to start upgrading firmware.
- 4. A Software Upgrade Proceeding screen will appear. The ZyAIR automatically reboots after a software upgrade.
- 5. After the ZyAIR finishes restarting, access the Web configurator again. Check the firmware version number in the System Status screen.

> All contents copyright © 2004 ZyXEL Communications Corporation.