\HELP\README.TXT

                    GN600 series Gigabit PCI Adapter
                  -------------------------------------

  Introduction
  ------------
  Thank you for purchasing the Gigabit PCI adapter. 
  The adapter card has been developed by combining the latest 1000BASE-T
  Gigabit Ethernet technology and peripheral component interface (PCI)
  local bus technology.

  Additionally,this adapter supports Wake-on-LAN feature in Windows 98SE,
  ME,2000,and XP allowing the system with a adapter card to be
  remotely configured.  This adapter card supports PCI rev 2.1
  systems which requires a 3-pin connector for system wake-up as well as
  PCI rev 2.2 system which can be awakened by the PME# signal on the PCI
  bus.There are two protocol boot rom supported. PXE and RPL protocol.
  For example,PXE for winnt4.0 , Windows 2000.
  When the system boot ,press <shift> + <F10> to change 
  the mode of bootstrap.

  Getting Started
  ---------------
  A DOS installation/help program, DIAG32.EXE, is provided for ease of setup 
  for normal users.  DIAG32.EXE will provide information on driver installation
  for the appropriate network operating systems.  

  To run the installation/help program, simply run DIAG32.EXE program in the 
  root directory of the driver disk.  (eg. A:\DIAG32<Enter>)

  
  If the network operating system you are using is not covered by the
  installation program, refer to the individual documentation provided
  for root directory.

  Revisions History
  -----------------
    Diskette Revision 1.10, 20030428
    ---------------------------------
    Initial release of the ZyXEL Communication Corporation GN650 series Gigabit PCI 
Adapter

  Trademarks
  ----------
  Microsoft, Microsoft Windows, Windows98, Windows NT,Windows 2000, Windows XP
  and Windows ME are registered trademarks of Microsoft Corporation.


