Upload Default Configuration File

There are two cases you need to upload the default configuration file to the Prestige, they are:

1. You forget the SMT password and want to reset the password to 1234.
2. You want to reset the configurations to defaults.

Please note that the default configuration file for the new ZyNOS is not compatible with the one for previous ZyNOS versions. So when upgrading your Pretige from the previous ZyNOS to please also update the default configuration file for the new ZyNOS.

- The procedure for uploading the configuration file via the console port is as follows.

1. Enter debug mode when powering on the Prestige using a terminal emulator
2. Enter 'ATUR3' to start the uploading.
3. Use X-modem protocol to transfer the configuration file.
4. Enter 'ATGO' to restart the Prestige.

- The procedure for uploading the configuration file using TFTP client program via LAN is as follows.

1. Use the TELNET client program in your PC to login to your Prestige.
2. Enter CI command 'sys stdio 0' in menu 24.8 to disable console idle timeout.
3. Start the TFTP client program and enter the Prestige's IP address.
4. To upload the configuration file, put the local configuration file to the Prestige as a remote file name 'rom-0

- Click here for the procedure to upload the configuration file using FTP via LAN or WAN

All contents copyright © 1999 ZyXEL Communications Corporation.