Documentation

Reference

RADIUS Support

RADIUS installation guide:

1. Get Radius application S/W and install first
2. Modify "Dictionary" file in Radius Folder and add the following entries:

`# Zyxel proprietary attributes` `ATTRIBUTE Zyxel-Callback-Option 192 integer` `VALUE Zyxel-Callback-Option None 0` `VALUE Zyxel-Callback-Option Optional 1` `VALUE Zyxel-Callback-Option Mandartory 2` `# Zyxel Callback phone number source` `ATTRIBUTE Zyxel-Callback-Phone-Source 193 integer` `VALUE Zyxel-Callback-Phone-Source Preconfigured 0` `VALUE Zyxel-Callback-Phone-Source User 1`

3. Modify "clients" file in Radius Folder and add Prestige IP like the following:

`# This file contains a list of clients which are allowed to make` `# authentication requests and their encryption key.` `# The first field is a valid hostname for the client.` `# The second field (seperated by blanks or tabs) is the encryption key.` `#` `#Client Name Key` `#---------------- -------------------` `#portmaster1 testing123` `203.66.113.187 key187`

Note:
The new client 203.66.113.187 is the Prestige router. The key 'key187' will be configured in SMT Menu 23.2.

4. Modify "users" file in Radius Folder and add the following entries:

`# Example PPP user with address Assigned by PortMaster. This is the most # commonly used entry in the users file.` `#` `# Username Password= " "` `#----------------------------------------------------------` `ray Password = "12345"` `#` `# Callback Example` `# Username Password= " "` `#----------------------------------------------------------` `test Password = "1234"` `ZyXEL-Callback-Option = Mandatory,` `ZyXEL-Callback-Phone-Source = Preconfigured` `CallBack-Number = "523444"``` ``

Username & Password for remote dial-in users

5. Run "RADIUS.EXE" to turn on radius service.

6. Setup Prestige as follows:

`Menu 23.2 - System Security - External Server` `Authentication Server:` `Active= Yes` `Type= RADIUS` `Server Address= 203.66.113.10` `Port #= 1645` `Key= key187`

Key Settings:

- Server Address--------IP address of RADIUS server, in the case, 203.66.113.10
- Port#------------------The port 1645 for RADIUS/UDP port
- Key-------------------The same key as configured in "Clients" in RADIUS folder

7. Please check prestige SMT menu 14 that no duplicate user name setting there compared to "users" file in step 4.

8. Then you can start the dial-in procedure from client side and have the RADIUS function done to do the password checking task for prestige.

Once you use "ray" as login name and "12345" as password, you can login sucessfully as a dial-in user.

All contents copyright © 1999 ZyXEL Communications Corporation.