ISDN Leased Line Connection

- Internet Access via ISDN Leased Line
- LAN-to-LAN Connection via ISDN Leased Line

Internet Access via ISDN Leased Line

This configuration illustrates an Internet Access over an ISDN leased line that is installed by the telco.

Key Settings in Prestige

- Menu 2 - ISDN Setup
- Menu 4 - Internet Access Setup

`Menu 2 - ISDN Setup` `Switch Type: DSS-1` `B Channel Usage= Leased/Unused` `Incoming Phone Numbers: ISDN Data =` `Advance Setup = No`

B Channel Usage:

- Set to Leased/Unused if you are using one 64K-leased line
- Set to Leased/Leased if you are using one 128K-leased lines
- Set to Leased/Switch if you are using one 64K-leased line and one switch line

The Prestige does not allow two leased lines to connect two different remote nodes. Therefore, if the Leased/Leased is configured in Menu 2, it allows a 128K-leased connection to a remote node or allows MP bundling to a remote node.

`Menu 4 - Internet Access Setup` `ISP's Name= hinet` `Pri Phone #= N/A` `Sec Phone #= N/A` `My Login= test` `My Password= ********` `My WAN IP Addr= 0.0.0.0` `NAT= SUA Only` `Address Mapping Set= N/A` `` `Telco Option:` `Transfer Type= Leased` `Multilink= Off` `Idle Timeout= 100`

Key Settings:

- My Login and My Password are the login information provided by ISP.
- Turn on SUA if you only have a single user Internet account.
- Enter the IP address assigned from ISP for Prestige, enter '0.0.0.0' if the IP is dynamically assigned during the PPP connection
- Set the 'Transfer Type' to 'Leased' for the ISDN leased-line connection

After saving this menu, you will be asked if you want to perform an Internet connection test. Select 'Yes' to perform the test. If the test fails, please check again the above settings again.

When you have configured and saved Menu 4, you should see that you have created a remote node in Menu 11. You can perform more advanced configuration options to this remote node in this menu.

LAN-to-LAN Connection via ISDN Leased Line

This configuration illustrates a LAN-to-LAN connection over an ISDN leased line that is subscribed from the telco.

- Key Settings in Prestige

- Menu 2 - ISDN Setup
- Menu 11 - Remote Node Setup

`Menu 2 - ISDN Setup` `Switch Type: DSS-1` `B Channel Usage= Leased/Unused` `Incoming Phone Numbers: ISDN Data =` `Advance Setup = No`

B Channel Usage:

- Set to Leased/Unused if you are using one 64K-leased line
- Set to Leased/Leased if you are using one 128K-leased lines
- Set to Leased/Switch if you are using one 64K-leased line and one switch line

The Prestige does not allow two leased lines to connect two different remote nodes. Therefore,
if the Leased/Leased is configured in Menu 2, it allows a 128K-leased connection to a remote node or allows MP bundling to a remote node.

`Menu 11.1 - Remote Node Profile` `Rem Node Name= LAN1 Edit PPP Options= No` `Active= Yes Rem IP Addr=` `140.113.1.1` `Call Direction= ******** Edit IP= No` `` `Incoming: Telco Option:` `Rem Login= Transfer Type=` `Leased` `Rem Password= Allocated Budget(min)=` `Rem CLID= N/A Period(hr)=` `Call Back= N/A Schedules=` `Outgoing: Carrier Access Code=` `My Login= test Nailed-Up Connection= No` `My Password= ******** Toll Period(sec)= 0` `Authen= CHAP/PAP Session Options:` `Pri Phone #= N/A Edit Filter Sets= No` `Sec Phone #= N/A Idle Timeout(sec)= 100` `Press ENTER to Confirm or ESC to Cancel:`

- Set the 'Transfer Type' to 'Leased' for the ISDN leased-line connection

All contents copyright © 1999 ZyXEL Communications Corporation.