Setup the Prestige as a DHCP Server

- What is DHCP Server?

DHCP stands for Dynamic Host Configuration Protocol. The P641supports the DHCP server function. When it is configured as a DHCP server, it assigns the IP addresses, DNS to the LAN clients. See figure 1.

- Setup the Prestige as a DHCP Client

1. Toggle the DHCP to Relay in menu 3.2 and enter the IP address of the DHCP server in the 'Relay Server Address' field.

`Menu 3.2 - TCP/IP and DHCP Ethernet Setup` `DHCP Setup DHCP= Relay` `Client IP Pool Starting Address= N/A` `Size of Client IP Pool= N/A` `Primary DNS Server= N/A` `Secondary DNS Server= N/A` `Relay Server Address= 192.168.1.2` `TCP/IP Setup:` `IP Address= 192.168.1.1` `IP Subnet Mask= 255.255.255.0` `RIP Direction= Both` `Version= RIP-1` `Press ENTER to Confirm or ESC to Cancel:`

All contents copyright © 1999 ZyXEL Communications Corporation.