Setup the Prestige as a DHCP Relay

- What is DHCP Relay?

DHCP stands for Dynamic Host Configuration Protocol. In addition to the DHCP server feature, the P650 supports the DHCP relay function. When it is configured as DHCP server, it assigns the IP addresses to the LAN clients. When it is configured as DHCP relay, it is reponsable for forwarding the requests and responses negotiating between the DHCP clients and the server. See figure 1.

- Setup the Prestige as a DHCP Client

1. Toggle the DHCP to Relay in menu 3.2 and enter the IP address of the DHCP server in the 'Relay Server Address' field.

`Menu 3.2 - TCP/IP and DHCP Ethernet Setup` `DHCP Setup DHCP= Relay` `Client IP Pool Starting Address= N/A` `Size of Client IP Pool= N/A` `Primary DNS Server= N/A` `Secondary DNS Server= N/A` `Relay Server Address= 192.168.1.2` `TCP/IP Setup:` `IP Address= 192.168.1.1` `IP Subnet Mask= 255.255.255.0` `RIP Direction= Both` `Version= RIP-1` `Press ENTER to Confirm or ESC to Cancel:`

All contents copyright © 2002 ZyXEL Communications Corporation.