VPN Routing between Branch Offices

1. Setup VPN in Branch Office A

2. Setup VPN in Branch Office B

3. Setup VPN in Headquarter

This page guides us how to setup VPN routing between branch offices through headquarter. So that whenever branch office A wants to talk to branch office B, headquarter plays as a VPN relay. Users can gain benefit from such application when the scale of branch offices is very large, because no additional VPN tunnels between branch offices are needed. In this support note, we skip the detailed configuration steps for Internet access and presume that you are familiar with basic ZyNOS VPN configuration.

As the figure shown below, each branch office have a VPN tunnel to headquarter, thus PCs in branch offices can access systems in headquarter via the tunnel. Through VPN routing, Prestige series now provide you a solution to let PCs in branch offices talk to each other through the existing VPN tunnels concentrated on the headquarter. This feature is available in Prestige10, Prestige50 and Prestige100.

The IP addresses we use in this example are as shown below.

Branch_A | Headquarter | Branch_B
WAN:202.3.1.1 LAN:192.168.3.1 | WAN:202.1.1.1 LAN:192.168.1.1 | WAN:202.2.1.1 LAN:192.168.2.1
LAN of Branch_A | LAN of Headquarter | LAN of Branch_B
192.168.3.0/24 | 192.168.1.0/24 | 192.168.2.0/24

1. Setup VPN in branch office A

Because VPN routing enables branch offices to talk to each other via tunnels concentrated on headquarter. In this step, we configure an IPSec rule in Prestige (Branch_A) for PCs behind branch office A to access both LAN segments of headquarter and branch office B. Because the LAN segments of headquarter and branch office B are continuous, we merge them into one single rule by including these two segments in Remote section. If by any chance, the two segments are not continuous, we strongly recommend you to setup different rules for these segments.

1. Click Advanced, and click VPN tab on the left.

2. On the SUMMARY menu, Select a policy to edit by clicking Edit.

3. On the CONFIGURE-IKE menu, check Active check box and give a name to this policy.

4. Give this VPN rule a name, Branch_A.

5. Select Key Management to IKE and Negotiation Mode to Main.

6. In Local section, select Address Type to Range Address, set IP Address Start to 192.168.3.0, and End to 192.168.3.255. This section covers the LAN segment of branch office A.

7. In Remot e section, select Address Type to Range Address, set IP Address Start to 192.168.1.0 and End to 192.168.2.255. This section covers the LAN segment of both headquarter and branch office B.

8. My IP Addr is the WAN IP of this Prestige, 202.3.1.1.

9. Set Secure Gateway Addr to the IP address of Headquarter, 202.1.1.1.

10. Select Encapsulation Mode to Tunnel.

11. Check the ESP check box. (AH can not be used in SUA/NAT case)

12. Select Encryption Algorithm to DES and Authentication Algorithm to SHA-1. These parameters are for IKE phase 2 negotiation. You can set more detailed configuration by pressing Advanced button.

13. Enter the key string 12345678 in the Pre-shared Key text box, and click Apply.

You can setup IKE phase 1 and phase 2 parameters by pressing Advanced button. Please make sure that parameters you set in this menu match with all the parameters with the correspondent VPN rule in headquarter.

2. Setup VPN in branch office B

Be very careful about the remote IP address in branch office B, because for systems behind branch office B want to systems behind branch office A and headquarter, we have to specify these two segments in Remote section. However if we include these two segments in one rule, the LAN segment of branch office B will be also included in this single rule, which means intercommunication inside branch office B will run into VPN tunnel. To avoid such situation, we need two separate rules to cover the LAN segment of branch office A and headquarter.

1. The first rule in Branch_ B.

This rule is for branch office B to access headquarter.

You can setup IKE phase 1 and phase 2 parameters by pressing Advanced button. Please make sure that parameters you set in this menu match with all the parameters with the correspondent VPN rule in headquarter.

2. The second rule in Branch_B

This rule is for branch office B to access branch office A.

You can setup IKE phase 1 and phase 2 parameters by pressing Advanced button. Please make sure that parameters you set in this menu match with all the parameters with the correspondent VPN rule in headquarter.

3. Setup VPN in Headquarter

1. The correspondent rule for Branch_A in headquarter

2. The correspondent rule for Branch_B_1 in headquarter

2. The correspondent rule for Branch_B_2 in headquarter