Configure 802.1x and WPA

- What is the WPA Functionality?
- Configuration for Access Point
- Configuration for your PC

- Introduction

What is WPA Functionality?

Wi-Fi Protected Access (WPA) is a subset of the IEEE 802.11i security specification draft. Key differences between WAP and WEP are user authentication and improved data encryption WAP applies IEEE 802.1x Extensible Authentication Protocol (EAP) to authenticate wireless clients using an external RADIUS database. You can not use the 662's local user database for WPA authentication purpose since the local user database uses MD5 EAP which can not to generate keys.

WPA improves data encryption by using Temporal Key Integrity Protocol (TKIP), Message Integrity Check and IEEE 802.1x. Temporal Key Integrity Protocol uses 128-bits keys that are dynamically generated and distributed by the authentication server. It includes a per-packet key mixing function, a Message Integrity Check (MIC) named Michael, an extend initialization vector (IV) with sequencing rules and a re-keying mechanism.

If you do not have an external RADIUS, server, you should use WPA-PSK (WPA Pre-Share Key) that only requires a single (identical) password entered into each access point, wireless gateway and wireless client. As long as the password match, a client will be granted access to a WLAN.

Here comes WPA-PSK Application example for your reference.

- Configuration for Access point

The IEEE 802.1x standard outlines enhanced security methods for both the authentication of wireless stations and encryption key management. Authentication cabn be done using local user database internal to the P662 (authenticate up to 32 users) or an external RADIUS server for an unlimited number of users.

1. To change your P662's authentication settings, click the wireless Wireless link under Advanced.

2. Select 802.1x/WPA tab.

3. choose Authentication Required from the Wireless Port Control.

4. Select the WAP-PSK in the Key Management Protocol field.

5. Type the Pre Shared Key in the Pre-Shared Key field.

6. select TKIP in the Group Data Privavy.

7. Click Apply to finish.

- Configuration for your PC

1. Double click on your wireless utility icon(here is the Centrion on Windows XP) in your windows task bar the utility will pop up on your windows screen.

2. Select the wireless card that you want to configure.

3. Select on from the Switch Radio.

4. choose Network option.

5. Add a new wireless profile.

6. Type the Profile Name and Network Name (SSID) in the field.

7. Click Next button.

8. Select WPA-PSK from the Network Authentication field.

9. Select TKIP from the Data Encryption field.

10. Type the Pre Share Key (8-63 character) in the Pass phrase field.

11. Click Finish to exit the Profile Wizard screen.

12. After you finished the profile settings, choose the profile you configured. Then, click Connect button to associate with the Access Point.

13. Click the General option, we will see the following information, that means the PC associated and authenticated with AP successfully.