LAN/WAN Packet Trace

The Prestige packet trace records and analyzes packets running on LAN and WAN interfaces. It is designed for users with technical backgrounds who are interested in the details of the packet flow on LAN or WAN end of Prestige. It is also very helpful for diagnostics if you have compatibility problems with your ISP or if you want to know the details of a packet for configuring a filter rule.

The format of the display is as following:

Packet:

`0 11880.160 ENET0-R[0062] TCP 192.168.1.2:1108->192.31.7.130:80`

[index] [timer/second][channel-receive/transmit][length] [protocol] [sourceIP/port] [destIP/port]

There are two ways to dump the trace:

1. Online Trace--display the trace real time on screen
2. Offline Trace--capture the trace first and display later

The details for capturing the trace in SMT menu 24.8 are as follows.

Online Trace

1. Trace LAN packet
2. Trace WAN packet

1. Trace LAN packet

1.1 Disable to capture the WAN packet by entering: `sys trcp channel mpoa00 none`
1.2 Enable to capture the LAN packet by entering: `sys trcp channel enet0 bothway`
1.3 Enable the trace log by entering: `sys trcp sw on & sys trcl sw on`
1.4 Display the brief trace online by entering: `sys trcd brief`
or
1.5 Display the detailed trace online by entering: `sys trcd parse`

`Example:`

`P642> sys trcp channel mpoa00 none` `p642> sys trcp channel enet0 bothway` `P642> sys trcp sw on` `P642> sys trcl sw on` `P642> sys trcd brief` `0 11880.160 ENET0-R[0062] TCP 192.168.1.2:1108->192.31.7.130:80` `1 11883.100 ENET0-R[0062] TCP 192.168.1.2:1108->192.31.7.130:80` `2 11883.330 ENET0-T[0058] TCP 192.31.7.130:80->192.168.1.2:1108` `3 11883.340 ENET0-R[0060] TCP 192.168.1.2:1108->192.31.7.130:80` `4 11883.340 ENET0-R[0339] TCP 192.168.1.2:1108->192.31.7.130:80` `5 11883.610 ENET0-T[0054] TCP 192.31.7.130:80->192.168.1.2:1108` `6 11883.620 ENET0-T[0102] TCP 192.31.7.130:80->192.168.1.2:1108` `7 11883.630 ENET0-T[0054] TCP 192.31.7.130:80->192.168.1.2:1108` `8 11883.630 ENET0-R[0060] TCP 192.168.1.2:1108->192.31.7.130:80` `9 11883.650 ENET0-R[0060] TCP 192.168.1.2:1108->192.31.7.130:80` `10 11883.650 ENET0-R[0062] TCP 192.168.1.2:1109->192.31.7.130:80` `p642> sys trcd parse` `---<0000>----------------------------------------------------------------` `LAN Frame: ENET0-RECV Size: 62/ 62 Time: 12089.790 sec` `Frame Type: TCP 192.168.1.2:1116->192.31.7.130:80` `Ethernet Header:` `Destination MAC Addr = 00A0C5921311` `Source MAC Addr = 0080C84CEA63` `Network Type = 0x0800 (TCP/IP)` `IP Header:` `IP Version = 4` `Header Length = 20` `Type of Service = 0x00 (0)` `Total Length = 0x0030 (48)` `Idetification = 0x330B (13067)` `Flags = 0x02` `Fragment Offset = 0x00` `Time to Live = 0x80 (128)` `Protocol = 0x06 (TCP)` `Header Checksum = 0x3E71 (15985)` `Source IP = 0xC0A80102 (192.168.1.2)` `Destination IP = 0xC01F0782 (192.31.7.130)` `TCP Header:` `Source Port = 0x045C (1116)` `Destination Port = 0x0050 (80)` `Sequence Number = 0x00BD15A7 (12391847)` `Ack Number = 0x00000000 (0)` `Header Length = 28` `Flags = 0x02 (....S.)` `Window Size = 0x2000 (8192)` `Checksum = 0xBEC3 (48835)` `Urgent Ptr = 0x0000 (0)` `Options =` `0000: 02 04 05 B4 01 01 04 02` `RAW DATA:` `0000: 00 A0 C5 92 13 11 00 80-C8 4C EA 63 08 00 45 00 .........L.c..E.` `0010: 00 30 33 0B 40 00 80 06-3E 71 C0 A8 01 02 C0 1F .03.@...>q......` `0020: 07 82 04 5C 00 50 00 BD-15 A7 00 00 00 00 70 02 ...\.P........p.` `0030: 20 00 BE C3 00 00 02 04-05 B4 01 01 04 02 .............` `---<0001>----------------------------------------------------------------` `LAN Frame: ENET0-XMIT Size: 58/ 58 Time: 12090.020 sec` `Frame Type: TCP 192.31.7.130:80->192.168.1.2:1116` `Ethernet Header:` `Destination MAC Addr = 0080C84CEA63` `Source MAC Addr = 00A0C5921311` `Network Type = 0x0800 (TCP/IP)` `IP Header:` `IP Version = 4` `Header Length = 20` `Type of Service = 0x00 (0)` `Total Length = 0x002C (44)` `Idetification = 0x57F3 (22515)` `Flags = 0x02` `Fragment Offset = 0x00` `Time to Live = 0xED (237)` `Protocol = 0x06 (TCP)` `Header Checksum = 0xAC8C (44172)` `Source IP = 0xC01F0782 (192.31.7.130)` `Destination IP = 0xC0A80102 (192.168.1.2)` `TCP Header:` `Source Port = 0x0050 (80)` `Destination Port = 0x045C (1116)` `Sequence Number = 0x4AD1B57F (1255257471)` `Ack Number = 0x00BD15A8 (12391848)` `Header Length = 24` `Flags = 0x12 (.A..S.)` `Window Size = 0xFAF0 (64240)` `Checksum = 0xF877 (63607)` `Urgent Ptr = 0x0000 (0)` `Options =` `0000: 02 04 05 B4` `RAW DATA:` `0000: 00 80 C8 4C EA 63 00 A0-C5 92 13 11 08 00 45 00 ...L.c........E.` `0010: 00 2C 57 F3 40 00 ED 06-AC 8C C0 1F 07 82 C0 A8 .,W.@...........` `0020: 01 02 00 50 04 5C 4A D1-B5 7F 00 BD 15 A8 60 12 ...P.\J.......`.` `0030: FA F0 F8 77 00 00 02 04-05 B4 ...w......` `---<0002>----------------------------------------------------------------` `LAN Frame: ENET0-RECV Size: 60/ 60 Time: 12090.210 sec` `Frame Type: TCP 192.168.1.2:1116->192.31.7.130:80` `Ethernet Header:` `Destination MAC Addr = 00A0C5921311` `Source MAC Addr = 0080C84CEA63` `Network Type = 0x0800 (TCP/IP)` `IP Header:` `IP Version = 4` `Header Length = 20` `Type of Service = 0x00 (0)` `Total Length = 0x0028 (40)` `Idetification = 0x350B (13579)` `Flags = 0x02` `Fragment Offset = 0x00` `Time to Live = 0x80 (128)` `Protocol = 0x06 (TCP)` `Header Checksum = 0x3C79 (15481)` `Source IP = 0xC0A80102 (192.168.1.2)` `Destination IP = 0xC01F0782 (192.31.7.130)` `TCP Header:` `Source Port = 0x045C (1116)` `Destination Port = 0x0050 (80)` `Sequence Number = 0x00BD15A8 (12391848)` `Ack Number = 0x4AD1B580 (1255257472)` `Header Length = 20` `Flags = 0x10 (.A....)` `Window Size = 0x2238 (8760)` `Checksum = 0xE8ED (59629)` `Urgent Ptr = 0x0000 (0)` `TCP Data: (Length=6, Captured=6)` `0000: 20 20 20 20 20 20` `RAW DATA:` `0000: 00 A0 C5 92 13 11 00 80-C8 4C EA 63 08 00 45 00 .........L.c..E.` `0010: 00 28 35 0B 40 00 80 06-3C 79 C0 A8 01 02 C0 1F .(5.@...<y......` `0020: 07 82 04 5C 00 50 00 BD-15 A8 4A D1 B5 80 50 10 ...\.P....J...P.` `0030: 22 38 E8 ED 00 00 20 20-20 20 20 20 "8....`

2. Trace WAN packet

1.1 Disable the capture of the LAN packet by entering: `sys trcp channel enet0 none`
1.2 Enable to capture the WAN packet by entering: `sys trcp channel mpoa00 bothway`
1.3 Enable the trace log by entering: `sys trcp sw on & sys trcl sw on`
1.4 Display the brief trace online by entering: `sys trcd brief`
or
1.5 Display the detailed trace online by entering: `sys trcd parse`

`Example:`

`P642> sys trcp channel enet0 none` `P642> sys trcp channel mpoa00 bothway p642> sys trcp sw on` `p642> sys trcl sw on` `P642> sys trcd brief` `0 12367.680 MPOA00-R[0070] UDP 202.132.155.95:520->202.132.155.255:520` `1 12370.980 MPOA00-T[0062] TCP 202.132.155.97:10261->192.31.7.130:80` `P642> sys trcd parse` `---<0000>----------------------------------------------------------------` `LAN Frame: MPOA00-RECV Size:1181/ 96 Time: 12387.260 sec` `Frame Type: TCP 192.31.7.130:80->202.132.155.97:10270` `Ethernet Header:` `Destination MAC Addr = 00A0C5921312` `Source MAC Addr = 00A0C5012345` `Network Type = 0x0800 (TCP/IP)` `IP Header:` `IP Version = 4` `Header Length = 20` `Type of Service = 0x00 (0)` `Total Length = 0x048B (1163)` `Idetification = 0xB139 (45369)` `Flags = 0x02` `Fragment Offset = 0x00` `Time to Live = 0xEE (238)` `Protocol = 0x06 (TCP)` `Header Checksum = 0xA9AB (43435)` `Source IP = 0xC01F0782 (192.31.7.130)` `Destination IP = 0xCA849B61 (202.132.155.97)` `TCP Header:` `Source Port = 0x0050 (80)` `Destination Port = 0x281E (10270)` `Sequence Number = 0xD3E95985 (3555285381)` `Ack Number = 0x00C18F63 (12685155)` `Header Length = 20` `Flags = 0x19 (.AP..F)` `Window Size = 0xFAF0 (64240)` `Checksum = 0x3735 (14133)` `Urgent Ptr = 0x0000 (0)` `TCP Data: (Length=1127, Captured=42)` `0000: DF 33 AF 62 58 37 52 3D-79 99 A5 3C 2B 59 E2 78 .3.bX7R=y..<+Y.x` `0010: A7 98 8F 3F A9 09 E4 0F-26 14 9C 58 3E 95 3E E7 ...?....&..X>.>.` `0020: FC 2A 4C 2F FB BE 2F FE-EF D0 .*L/../...` `RAW DATA:` `0000: 00 A0 C5 92 13 12 00 A0-C5 01 23 45 08 00 45 00 ..........#E..E.` `0010: 04 8B B1 39 40 00 EE 06-A9 AB C0 1F 07 82 CA 84 ...9@...........` `0020: 9B 61 00 50 28 1E D3 E9-59 85 00 C1 8F 63 50 19 .a.P(...Y....cP.` `0030: FA F0 37 35 00 00 DF 33-AF 62 58 37 52 3D 79 99 ..75...3.bX7R=y.` `0040: A5 3C 2B 59 E2 78 A7 98-8F 3F A9 09 E4 0F 26 14 .<+Y.x...?....&.` `0050: 9C 58 3E 95 3E E7 FC 2A-4C 2F FB BE 2F FE EF D0 .X>.>..*L/../...`

Offline Trace

1. Trace LAN packet
2. Trace WAN packet

1. Trace LAN packet

1.1 Disable the capture of the WAN packet by entering: `sys trcp channel mpoa00 none`
1.2 Enable the capture of the LAN packet by entering: `sys trcp channel enet0 bothway`
1.3 Enable the trace log by entering: `sys trcp sw on & sys trcl sw on`
1.4 Wait for packet passing through the Prestige over LAN
1.5 Disable the trace log by entering: `sys trcp sw off & sys trcl sw off`
1.6 Display the trace briefly by entering: `sys trcp brief`
1.7 Display specific packets by using: `sys trcp parse <from_index> <to_index>`

2. Trace WAN packet

1.1 Disable the capture of the LAN packet by entering: `sys trcp channel enet0 none`
1.2 Enable the capture of the WAN packet by entering: `sys trcp channel mpoa00 bothway`
1.3 Enable the trace log by entering: `sys trcp sw on & sys trcl sw on`
1.4 Wait for packet passing through the Prestige over WAN
1.5 Disable the trace log by entering: `sys trcp sw off & sys trcl sw off`
1.6 Display the trace briefly by entering: `sys trcp brief`
1.7 Display specific packets by using: `sys trcp parse <from_index> <to_index>`

All contents copyright 2002 ZyXEL Communications Corporation.