Setup the Prestige for PPPoE Connections

- Introduction

PPP over Ethernet is an IETF draft standard specifying how a host personal computer (PC) interacts with a broadband modem (i.e. xDSL, cable, wireless, etc.) to achieve access to the high-speed data networks via a familiar PPP dialer such as 'Dial-Up Networking' user interface. PPPoE supports a broad range of existing applications and service including authentication, accounting, secure access and configuration management. There are several major service providers running evaluations of PPPoE today. When the Prestige is deployed in such a setup, it must appear as a single host to the access concentrator. Before using PPPoE feature of the Prestige, please make sure your ISP supports PPPoE.

- Setup the Prestige for Internet Access using PPPoE

`Menu 4 - Internet Access Setup` `ISP's Name= ChangeME` `Encapsulation= PPPoE` `Multiplexing= LLC-based` `VPI #= 0` `VCI #= 35``` `ATM QoS Type= CBR Peak Cell Rate (PCR)= 0 Sustain Cell Rate (SCR)= 0 Maximum Burst Size (MBS)= 0` `My Login= user@domain` `My Password= ********` `` `Idle Timeout (sec)= 0 IP Address Assignment= Dynamic IP Address= N/A Network Address Translation= SUA Only Address Mapping Set= N/A` `Press ENTER to Confirm or ESC to Cancel:`

Key Settings for making a PPPoE connection:

Option | Description
Encapsulation | Set 'PPPoE' as the encapsulation.
Multiplexing | Toggle to select the method of multiplexing used by your ISP.
VPI# | Enter the VPI number that the telephone company gives to you.
VCI# | Enter the VCI number that the telephone company gives to you.
My Login | Enter the login name that your ISP gives to you. If you are using PPPoE encapsulation, then this field must be of the form user@domain where domain identifies your ISP.
My Password | Enter the password associated with the login name above.
Network Address Translation | Select 'Full Feature' if you have multiple public WAN IP addresses for your Prestige. The SMT uses the address mapping set that you configure and enter in the Address Mapping Set field (menu 15.1. When you select 'SUA Only', the SMT uses Address Mapping Set 255 (menu 15.1). Choose SUA Only if you have just one public WAN IP address for your Prestige.
IP Address Assignment | Choose 'Dynamic' if the ISP provides the IP dynamically, otherwise choose 'Static'.
IP Address | Enter the IP address supplied by your ISP if applicable.

All contents copyright © 2003 ZyXEL Communications Corporation.