# AVR32 AP7 - SSC Driver for I2S Documentation

## Introduction

This documents data structures, functions, variables, defines, enums, and typedefs in the software for application note AVR32x. It also gives an example of the usage of the SSC driver generating I2S output.

## Main Files

- ssc_i2s.c: SSC I2S driver
- ssc_i2s.h: SSC I2S driver header file
- ssc_i2s_example.c: SSC I2S example application.

## Compilation Info

This software was written for the GNU GCC for AVR32 and IAR Systems compiler for AVR32. Other compilers may or may not work.

## Device Info

All AVR32 devices with an SSC module can be used. This example has been tested with the following setup:

- STK1000 with a oscilloscope probing the I2S signals.

## Setup Information

CPU speed: 20 MHz

## Application Usage

### Master mode

## Contact Information

For further information, visit Atmel AVR32.
Support and FAQ: http://support.atmel.no/