o Modem Dialout Terminal: xc command

Usage: miterm [ -s speed ] [-l device] 
        -l device       Use 'device' as the modem port
        -s speed      	115200, 38400 and 2400 

Examples:

			# miterm  -l /dev/ttyS1

Test  the serial line with:

			ATZ --> response: OK

Dial a phone number with:

			ATX3
			ATDT05872....
Exit with:

		~.

The symbol ~ is ALT-126, of course.

