From: Henri VIRET <hviret@compuserve.com>
Subject: RDPS Addon for MuLinux ...?!?
Sender: Henri VIRET <hviret@compuserve.com>
To: Michele ANDREOLI <m.andreoli@tin.it>

	Configuring Windows to connect to
	a Mulinux RDPS (Remote Dialin PPP Server)
	=========================================

To use the Remote Dialin PPP Server with Windows 95/98 Dial-up 
networking, configure as follows: 

  From the Start menu, open the dial-up networking folder.
  Select "Make New Connection" to start the wizard. 

  Name the connection appropriately, select and check your modem
configuration
  Select "Next", then enter the phone number 

  Select "Next" and confirm to finish the wizard. 


  Right click on the Icon for the connection just created, and select
"Properties". 

  Select Server type, and Set the type of dial-up to PPP, enable 
log onto  network,
  software compression, and TCP/IP protocols. 

  Select the TCP/IP Settings button, and select 
Server Assigned IP and DNS addresses. 

  Select IP header compression and default gateway.
  Click OK twice to return to  the General Tab. 


  Test the connection by double-clicking the dial-in icon. 

  When the terminal window comes up, enter the login name and password
  for the PPP login ( use the same values as in the RDPS setup on Mulinux ).
  Click to establish the connection. 

  The PPP link should establish itself and be operational ... 


 Enjoy ...

