# Netzwerken unter FreeDOS - Netzwerk

      Netzwerke erlauben es zwei oder mehr Computern, sich zu verbinden und
      Informationen miteinander zu teilen, z.B. ueber das Internet und einen
      Webbrowser. Um verbunden zu werden, brauchen Sie entweder ein Modem
      oder eine Ethernet Karte (Netzwerkkarte). Wenn Sie Ethernet waehlen,
      benoetigen Sie einen unterstuetzenden Treiber, wie z.B. Crynwr, ODI
      oder NDIS. Das gebraeuchlichste Protokoll ist TCP/IP, aber viele
      Netzwerke unterstuetzen auch IPX/SPX. Um Daten mit anderen Systemen
      zu teilen, werden Sie NFS oder CIFS benoetigen.
        * Hauptartikel: Netzwerken unter FreeDOS

#### [Hauptseite] [oben] [Externe Links]

## Externe Links

        * Bart's Network Boot Disk ver 2.7 (Bart Lagerweij, vgl.:
          http://www.nu2.nu/bootdisk/network/)
        * DOS applications for Internet Use (Michael Bernardi, vgl.:
          http://www.dendarii.co.uk/FAQs/dos-apps.html)
        * DOS-Meta FAQ: Useful information for DOS users (Michael Bernardi,
          vgl.: http://www.dendarii.co.uk/FAQs/dos-meta_faq.html)

#### [Hauptseite] [oben] (Externe Links)

      Copyright © 2007 Ulrich Hansen, Mainz (Germany), 2010 an die
      FreeDOS-Hilfe angepasst von W.Spiegl.
      Weitergehende Informationen finden Sie hier.

      Permission is granted to copy, distribute and/or modify this document
      under the terms of the GNU Free Documentation License, Version 1.1 or
      any later version published by the Free Software Foundation.
      A copy of the license is included in the section entitled
      "GNU Free Documentation License"