# Command: ;

      ';' marks the config.sys line as a comment. ';' has the same effect
      as 'REM'.
      ';' is a CONFIG.SYS / FDCONFIG.SYS command.

## Syntax:

      ; [comment]
      REM [comment]

#### [Main menu] [top] (Syntax) [Options] [Comments] [Examples] [See also] [File]

## Options:

      comment  any comment you want to add to remember why you did this or
               that; can also be a command, which shall not be executed
               (maybe for test purposes).

#### [Main menu] [top] [Syntax] (Options) [Comments] [Examples] [See also] [File]

## Comments:

      ';' and 'REM' provide the ability to place comments within the
      configuration file. The text following the ';' or 'REM' until the end
      of the line is reached is ignored. This may also be used to temporarily
      disable loading a particular device or other option.
      ';' is a command internal to kernel.sys and needs no other file
      in order to work.

#### [Main menu] [top] [Syntax] [Options] (Comments) [Examples] [See also] [File]

## Examples:

      IN CONFIG.SYS / FDCONFIG.SYS:
        REM DOS=HIGH,UMB  has the same effect!
        ;DOS=HIGH,UMB     has the same effect!

#### [Main menu] [top] [Syntax] [Options] [Comments] (Examples) [See also] [File]

## See also:

      !
      ?
      config.sys
      fdconfig.sys
      rem

#### [Main menu] [top] [Syntax] [Options] [Comments] [Examples] (See also) [File]

## File:

      Please read this command's lsm file also.
      You will find the updated version (internet) here and
      the version described in this manual page here.
      The lsm file contains information about the name of the programmer,
      the download site, and some other command related information.

#### [Main menu] [top] [Syntax] [Options] [Comments] [Examples] [See also] (File)

      Copyright © 2008 W. Spiegl.

      This file is derived from the FreeDOS Spec Command HOWTO.
      See the file H2Cpying for copying conditions.